{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["製品仕様(PTGL 突入電流抑制)","品番一覧"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"製品仕様(PTGL 突入電流抑制)","index":0,"n_rows":58,"n_cols":28,"rows_kept":58,"cut":false,"hidden":false,"merged":[[2,3,2,5],[5,23,5,24],[5,25,5,26],[5,3,5,5],[5,6,5,7],[5,11,5,13],[5,14,5,16],[5,17,5,19],[5,20,5,22]]}
[null,null,null,"Comparison Data of PTGL Series (Inrush Current limitting Type)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PSE-21THM-0048"]
[]
[null,"品番検索\nP/N Search",null,null,null,null,{"$f":"VLOOKUP(D3,品番一覧!B2:C29,2,FALSE)","v":{"$error":"#N/A"}}]
[]
[]
["メーカー\nMaker","品番\nPart Number","グルーピング","抵抗値\nResistance",null,null,"最大電圧\nMax. Voltage",null,"最大突入電流\nMax. Inrush \nCurrent","最大充電ｴﾈﾙｷﾞｰ\nMax. Energy","熱容量\n(Cth)","外径寸法 max.(mm)\nBody Size",null,null,"製品厚み max.(mm)\nBody Thikness",null,null,"ﾘｰﾄﾞ線間隔(mm)\nPin Spacing",null,null,"ﾘｰﾄﾞ線径 (mm)\nLead wire diameter",null,null,"使用温度範囲\nOperating Temp. range",null,"実装後の保存温度範囲\nStrage Temp. range after Mouting",null,"備考\nRemarks"]
[null,null,"No.","Ω","- %","+%","value","dimension","value","value","J/K","Value","-","+","Value","-","+","Value","-","+","Value","-","+","Min. (℃)","Max.(ﾟC)","Min. (℃)","Max.(ﾟC)"]
["Murata","PTGL07AS121M0B51A0",1,120,20,20,280,"Vrms.","8.46Ao-p","-","-",7.8,"-","-",6,"-","-",5,0.3,0.8,0.6,0.05,0.05,-40,105,-40,125,"-"]
["Murata","PTGL07AS121M0B51B0",1,120,20,20,280,"Vrms.","8.46Ao-p","-","-",7.8,"-","-",6,"-","-",5,1.5,1.5,0.6,0.05,0.05,-40,105,-40,125,"-"]
["TDK/EPCOS","B59771C0120A070",1,120,25,25,260,"Vrms.",2.8,"-",0.6,9,"-","-",7.5,"-","-",5,"-","-",0.6,"-","-",-20,85,-40,125,"-"]
["Murata","PTGL07AS121M0N51A0",2,120,20,20,280,"Vrms.","8.46Ao-p","-","-",7.8,"-","-",6,"-","-",5,0.3,0.8,0.5,0.05,0.05,-40,105,-40,125,"-"]
["Murata","PTGL7SAS121M0N51A0",2,120,20,20,140,"Vrms.","4.23Ao-p","9.3J @100ﾟC","-",7.8,"-","-",6,"-","-",5,0.3,0.8,0.5,0.05,0.05,-40,105,-40,125,"-"]
["Murata","PTGL07AS121M0N51B0",2,120,20,20,280,"Vrms.","8.46Ao-p","-","-",7.8,"-","-",6,"-","-",5,1.5,1.5,0.5,0.05,0.05,-40,105,-40,125,"-"]
["TDK/EPCOS","B59771C0120A070",2,120,25,25,260,"Vrms.",2.8,"-",0.6,9,"-","-",7.5,"-","-",5,"-","-",0.6,"-","-",-20,85,-40,125,"-"]
["Murata","PTGL07AS181M0N51A0",3,180,20,20,280,"Vrms.","6.22Ao-p","-","-",7.3,"-","-",6,"-","-",5,0.3,0.8,0.5,0.05,0.05,-40,105,-40,125,"-"]
["Murata","PTGL07AS181M0N51B0",3,180,20,20,280,"Vrms.","6.22Ao-p","-","-",7.3,"-","-",6,"-","-",5,1.5,1.5,0.5,0.05,0.05,-40,105,-40,125,"-"]
["Murata","PTGL07AS181M0N52A0",3,180,20,20,280,"Vrms.","6.22Ao-p","-","-",7.3,"-","-",6,"-","-",5,0.3,0.8,0.5,0.05,0.05,-40,105,"-","-","-"]
["TDK/EPCOS","B59772C0120A070",3,150,25,25,260,"Vrms.",2.8,"-",0.6,9,"-","-",7.5,"-","-",5,"-","-",0.6,"-","-",-20,85,-40,125,"-"]
["Murata","PTGL14AS330H0B02BZ",4,33,25,25,280,"Vrms.","39Ao-p","109.7J @60ﾟC",1.4,16,"-","-",6.5,"-","-",10,1.5,1.5,0.6,0.05,0.05,-20,85,-40,125,"-"]
["TDK/EPCOS","B59751C0120A070",4,50,25,25,280,"Vrms.",4,"-",1.4,13,"-","-",7.5,"-","-",5,"-","-",0.6,"-","-",-20,85,-40,125,"-"]
["Vishay","PTCEL13R600LBE",4,60,30,30,350,"Vrms.",40,"-",1.45,13.5,"-","-",7,"-","-",5,0.8,0.8,0.6,0.06,0.06,-40,105,-40,165,"-"]
["Murata","PTGL14AS470H0B02BZ",5,47,25,25,280,"Vrms.","27Ao-p","106.9J @60ﾟC",1.4,16,"-","-",6.5,"-","-",10,1.5,1.5,0.6,0.05,0.05,-20,85,-40,125,"-"]
["Murata","PTGL14AS470H0B02B2",5,47,25,25,280,"Vrms.","27Ao-p","106.9J @60ﾟC",1.4,16,"-","-",6.5,"-","-",10,1.5,1.5,0.6,0.05,0.05,-20,85,-40,125,"Lead Length 25mm"]
["Murata","PTGL14AS470H0B72BZ",5,47,25,25,280,"Vrms.","27Ao-p","1430μF@230vrms.\n @75ﾟC",1.4,16,"-","-",6.5,"-","-",7.5,1.5,1.5,0.6,0.05,0.05,-20,85,-40,125,"-"]
["Murata","PTGL14AS470H0D75BZ",5,47,25,25,280,"Vrms.","27Ao-p","1430μF @230vrms. \n@75ﾟC",1.4,16,"-","-",6.5,"-","-",7.5,1.5,1.5,0.8,0.05,0.05,-20,85,-40,125,"-"]
["Murata","PTGL14AS470H0D76AZ",5,47,25,25,280,"Vrms.",27,"106.9J @60ﾟC",1.4,16,"-","-",6.5,"-","-",7.5,1.5,1.5,0.8,0.05,0.05,-20,85,-40,125,"-"]
["Murata","PTGL14AS470H0D76BZ",5,47,25,25,280,"Vrms.",27,null,1.4,16,"-","-",6.5,"-","-",7.5,1.5,1.5,0.8,0.05,0.05,-20,85,-40,125,"-"]
["TDK/EPCOS","B59751C0120A070",5,50,25,25,280,"Vrms.",4,"-",1.4,13,"-","-",7.5,"-","-",5,"-","-",0.6,"-","-",-20,85,-40,125,"-"]
["Thinking","PPL11500*A2C8",5,50,"-","-",380,"Vrms.","-","54J@60ﾟC",1.4,"10.5to13","-","-","5to7.5","-","-",5,1,1,0.6,0.02,0.02,-20,85,-40,125,"'*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCEL13R600LBE",5,60,30,30,350,"Vrms.",40,"-",1.45,13.5,"-","-",7,"-","-",5,0.8,0.8,0.6,0.06,0.06,-40,105,-40,165,"-"]
["Murata","PTGL16AS330H0B02BZ",6,33,25,25,280,"Vrms.","39Ao-p","140J @60ﾟC",1.8,18,"-","-",6.5,"-","-",10,1.5,1.5,0.6,0.05,0.05,-20,85,-40,125,"-"]
["TDK/EPCOS","B59451C1130B070",6,56,25,25,440,"Vrms.",12,"-",2.1,15,"-","-",7.5,"-","-",5,"-","-",0.8,"-","-",-20,85,-40,125,"-"]
["Vishay","PTCEL17R600MBE",6,60,30,30,440,"Vrms.",40,"-",2.2999999999999998,17,"-","-",7.5,"-","-",5,0.8,0.8,0.8,0.08,0.08,-40,105,-40,165,"-"]
["Murata","PTGL16AS470H0B72BZ",7,47,25,25,280,"Vrms.","15Ao-p","99J @25ﾟC",1.8,17,"-","-",6.5,"-","-",7.5,1.5,1.5,0.6,0.05,0.05,-20,85,-40,125,"-"]
["Murata","PTGL16AS470H0B02BZ",7,47,25,25,280,"Vrms.","27Ao-p","130.8J @60ﾟC",1.8,18,"-","-",6.5,"-","-",10,1.5,1.5,0.6,0.05,0.05,-40,85,-40,125,"-"]
["Murata","PTGL16AS470H0D71AZ",7,47,25,25,280,"Vrms.","27Ao-p","130.8J @60ﾟC",1.8,18,"-","-",6.5,"-","-",7.5,1.5,1.5,0.8,0.05,0.05,-35,95,-40,125,"-"]
["TDK/EPCOS","B59412C1130B070",7,120,25,25,480,"Vrms.",7,"-",2.1,15,"-","-",7.5,"-","-",5,"-","-",0.8,"-","-",-20,85,-40,125,"-"]
["Thinking","PPL20330*A3B7",7,33,"-","-",270,"Vrms.","-","186J@60ﾟC",3.8,"19.5to22","-","-","6.5 t010.7","-","-",10,1,1,1,0.02,0.02,-20,85,-40,125,"'*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCEL17R600MBE",7,60,30,30,440,"Vrms.",40,"-",2.2999999999999998,17,"-","-",7.5,"-","-",5,0.8,0.8,0.8,0.08,0.08,-40,105,-40,165,"-"]
["Murata","PTGL16AS680H0B02BZ",8,68,25,25,280,"Vrms.","19Ao-p","130.8J @60ﾟC",1.8,18,"-","-",6.5,"-","-",10,1.5,1.5,0.6,0.05,0.05,-20,85,-40,125,"-"]
["TDK/EPCOS","B59451C1130B070",8,56,25,25,440,"Vrms.",12,"-",2.1,15,"-","-",7.5,"-","-",5,"-","-",0.8,"-","-",-20,85,-40,125,"-"]
["Vishay","PTCEL17R600MBE",8,60,30,30,440,"Vrms.",40,"-",2.2999999999999998,17,"-","-",7.5,"-","-",5,0.8,0.8,0.8,0.08,0.08,-40,105,-40,165,"-"]
["Thinking","PPL16500*A2B7",8,65,"-","-",270,"Vrms.","-","97J@60ﾟC",2.2999999999999998,"15.5to18","-","-","5to7.5","-","-",10,1,1,1,0.02,0.02,-20,85,-40,125,"'*= Resistance Torelance ex.) M,H,N"]
["Murata","PTGL16AS101H0B02BZ",9,100,25,25,280,"Vrms.","13Ao-p","130.8J @60ﾟC",1.8,18,"-","-",6.5,"-","-",10,1.5,1.5,0.6,0.05,0.05,-20,85,-40,125,"-"]
["Murata","PTGL16AS101H0D02BZ",9,100,25,25,280,"Vrms.","-","-",1.8,18,"-","-",6.5,"-","-",10,1.5,1.5,0.8,0.05,0.05,-20,85,-40,125,"-"]
["Murata","PTGL16AS101H0D71AZ",9,100,25,25,280,"Vrms.","13Ao-p","130.8J @60ﾟC",1.8,18,"-","-",6.5,"-","-",7.5,0.5,0.5,0.8,0.05,0.05,-20,85,-40,125,"-"]
["TDK/EPCOS","B59412C1130B070",9,120,25,25,480,"Vrms.",7,"-",2.1,15,"-","-",7.5,"-","-",5,"-","-",0.8,"-","-",-20,85,-40,125,"-"]
["Thinking","PPL14121*A3D4",9,120,"-","-",440,"Vrms.","-","103J@60ﾟC",2.1,"12.5to15","-","-","5to7.5","-","-",5,1,1,0.6,0.02,0.02,-20,85,-40,125,"'*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCEL17R121NBE",9,120,30,30,460,"Vrms.",40,"-",2.2999999999999998,17,"-","-",7.5,"-","-",5,0.8,0.8,0.8,0.08,0.08,-40,105,-40,165,"-"]
["Murata","PTGL20AS330H0D02BZ",10,33,25,25,280,"Vrms.","39Ao-p","181.7J @60ﾟC",2.6,22,"-","-",6.5,"-","-",10,1.5,1.5,0.8,0.05,0.05,-20,85,-40,125,"-"]
["Murata","PTGL20AS330H0P02BZ",10,33,25,25,280,"Vrms.","13Ao-p","130.8J @60ﾟC",2.6,22,"-","-",6.5,"-","-",10,1.5,1.5,0.6,0.05,0.05,-20,85,-40,125,"-"]
["TDK/EPCOS","B59451C1130B070",10,56,25,25,440,"Vrms.",12,"-",2.1,15,"-","-",7.5,"-","-",5,"-","-",0.8,"-","-",-20,85,-40,125,"-"]
["Thinking","PPL20330*A3B7",10,33,"-","-",270,"Vrms.","-","186J@60ﾟC",3.8,"19.5to22","-","-","6.5 t010.7","-","-",10,1,1,1,0.02,0.02,-20,85,-40,125,"'*= Resistance Torelance ex.) M,H,N"]
["Murata","PTGL20AS470H0D02BZ",11,47,25,25,280,"Vrms.","27Ao-p","181.7J @60ﾟC",2.6,22,"-","-",6.5,"-","-",10,1.5,1.5,0.8,0.05,0.05,-20,85,-40,125,"-"]
["Murata","PTGL20AS470H0D76AZ",11,47,25,25,280,"Vrms.",27,"-",2.6,22,"-","-",6.5,"-","-",7.5,1.5,1.5,0.8,0.05,0.05,-20,85,-40,125,"-"]
["Murata","PTGL20AS470H0P02BZ",11,47,25,25,280,"Vrms.",27,"-",2.6,22,"-","-",6.5,"-","-",10,1.5,1.5,0.6,0.05,0.05,-20,85,-40,125,"-"]
["Vishay","PTCEL17R600MBE",11,60,30,30,440,"Vrms.",40,"-",2.2999999999999998,17,"-","-",7.5,"-","-",5,0.8,0.8,0.8,0.08,0.08,-40,105,-40,165,"-"]
["Thinking","PPL20330*A3B7",11,33,"-","-",270,"Vrms.","-","186J@60ﾟC",3.8,"19.5to22","-","-","6.5 t010.7","-","-",10,1,1,1,0.02,0.02,-20,85,-40,125,"'*= Resistance Torelance ex.) M,H,N"]

{"sheet":"品番一覧","index":1,"n_rows":29,"n_cols":3,"rows_kept":29,"cut":false,"hidden":true,"merged":[]}
["メーカー\nMaker","品番\nPart Number","グルーピング"]
["Murata","PTGL07AS121M0B51A0",1]
["Murata","PTGL07AS121M0B51B0",1]
["Murata","PTGL07AS121M0N51A0",2]
["Murata","PTGL07AS121M0N51B0",2]
["Murata","PTGL07AS181M0N51A0",3]
["Murata","PTGL07AS181M0N51B0",3]
["Murata","PTGL07AS181M0N52A0",3]
["Murata","PTGL14AS330H0B02BZ",4]
["Murata","PTGL14AS470H0B02B2",5]
["Murata","PTGL14AS470H0B02BZ",5]
["Murata","PTGL14AS470H0B72BZ",5]
["Murata","PTGL14AS470H0D75BZ",5]
["Murata","PTGL14AS470H0D76AZ",5]
["Murata","PTGL14AS470H0D76BZ",5]
["Murata","PTGL16AS101H0B02BZ",9]
["Murata","PTGL16AS101H0D02BZ",9]
["Murata","PTGL16AS101H0D71AZ",9]
["Murata","PTGL16AS330H0B02BZ",6]
["Murata","PTGL16AS470H0B02BZ",7]
["Murata","PTGL16AS470H0B72BZ",7]
["Murata","PTGL16AS470H0D71AZ",7]
["Murata","PTGL16AS680H0B02BZ",8]
["Murata","PTGL20AS330H0D02BZ",10]
["Murata","PTGL20AS330H0P02BZ",10]
["Murata","PTGL20AS470H0D02BZ",11]
["Murata","PTGL20AS470H0D76AZ",11]
["Murata","PTGL20AS470H0P02BZ",11]
["Murata","PTGL7SAS121M0N51A0",2]