{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["製品仕様(PTGL 過電流保護)","品番一覧"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"製品仕様(PTGL 過電流保護)","index":0,"n_rows":606,"n_cols":32,"rows_kept":606,"cut":false,"hidden":false,"merged":[[5,21,5,23],[5,24,5,26],[5,27,5,28],[5,29,5,30],[5,18,5,20],[5,15,5,17],[2,3,2,5],[5,3,5,4],[5,5,5,7],[5,8,5,10],[5,11,5,13]]}
[null,null,null,"Comparison Data of PTGL Series (Overcurrent Protection Type)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PSE-21THM-0047"]
[]
[null,"品番検索\nP/N Search",null,null,null,null,{"$f":"VLOOKUP(D3,品番一覧!B2:C351,2,FALSE)","v":{"$error":"#N/A"}}]
[]
[]
["メーカー\nMaker","品番\nPart Number","グルーピング","最大電圧\nMax. Voltage",null,"保持電流(mA)\nHold Current",null,null,"トリップ電流(mA)\nTrip Current",null,null,"抵抗値\nResistance",null,null,"最大電流\nMax. Current","外径寸法(mm)\nBody Size",null,null,"製品厚み(mm)\nBody Thikness",null,null,"ﾘｰﾄﾞ線間隔(mm)\nPin Spacing",null,null,"ﾘｰﾄﾞ線径 (mm)\nLead wire diameter",null,null,"使用温度範囲\nOperating Temp. range",null,"実装後の保存温度範囲\nStrage Temp. range after Mouting",null,"備考\nRemarks"]
[null,null,"No.","Value","dimensions","25℃","60℃","85℃","25℃","-10℃","-30℃","Ω","-%","+%","A","Value","-","+","Value","-","+","Value","-","+","Value","-","+","Min. (℃)","Max.(ﾟC)","Min. (℃)","Max.(ﾟC)"]
["Murata","PTGL3SAR1R8M1E51A0",1,16,"VDC","-","-",175,"-","-",575,1.8,20,20,1.5,4.2,"-","-",2.5,"-","-",5,0.3,0.8,0.4,0.05,0.05,-30,85,-40,95,"-"]
["Murata","PTGL3SAR1R8K1E51A0",1,16,"VDC","-","-",165,"-","-",545,1.8,10,10,1.5,5.5,"-","-",2.5,"-","-",5,0.3,0.8,0.4,0.03,0.03,-30,85,"-","-","Special specification type"]
["Maximum Tech.","PTDD03N2-1R8M160",1,16,"V","-","-","190(80ﾟC)","-","-",760,1.8,20,20,1.8,5,"-","-","-","-","-",5,"-","-",0.5,"-","-","-","-","-","-","-"]
["Murata","PTGL05BA1R8M1B51A0",2,16,"Vrms.","－",285,"-","-",850,"-",1.8,20,20,2,6,"-","-",4,"-","-",5,0.2,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL05BA1R8M1B51B0",2,16,"Vrms.","－",285,"-","-",850,"-",1.8,20,20,2,6,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59985C0160A070",2,20,"Vrms.",300,240,201,600,690,"-",4.5999999999999996,25,25,1,6.5,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,85,-40,125,"-"]
["Nichicon","ZPC11CE2R2K",2,16,"V","-",300,"-","-",760,"-",2.2000000000000002,20,20,2.1,5.5,"-","-",3,"-","-",5,"-","-",0.5,"-","-","-","-","-","-","-"]
["Murata","PTGL03AR2R0Q1B53A0",3,16,"VDC","-","-",250,"-","-",790,2,25,10,2.6,5,"-","-",4,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-40,95,"-"]
["Murata","PTGL03AR2R0Q1B53B0",3,16,"VDC","-","-",250,"-","-",790,2,25,10,2.6,5,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,95,"-"]
["Thinking","PPL081R8*A212",3,12,"Vrms.",450,"-","-",900,"-","-",1.8,"-","-",3,"7.5to10","-","-","1.5to3.5","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL07H411D*E",3,30,"Vrms.",410,328,254.2,615,725.69999999999993,787.2,3,20,20,4.5,7,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL3SAR2R5M1N51A0",4,16,"VDC","-","-",123,"-","-",540,2.5,20,20,1.5,4.2,"-","-",2.5,"-","-",5,0.3,0.8,0.5,0.05,0.05,-30,85,"-","-","-"]
["Murata","PTGL3SAR2R5M1N51B0",4,16,"VDC","-","-",123,"-","-",540,2.5,20,20,1.5,4.2,"-","-",2.5,"-","-",5,1.5,1.5,0.5,0.05,0.05,-30,85,"-","-","-"]
["Murata","PTGL3SAR2R5M1N53A0",4,16,"VDC","-","-",120,"-","-",550,2.5,20,20,1.5,3.8,0.4,0.4,1.8,0.5,0.5,5,0.3,0.8,0.5,0.05,0.05,-40,85,"-","-","-"]
["Murata","PTGL3SAR2R5M1N53B0",4,16,"VDC","-","-",120,"-","-",550,2.5,20,20,1.5,3.8,0.4,0.4,1.8,0.5,0.5,5,1.5,1.5,0.5,0.05,0.05,-40,85,"-","-","-"]
["Maximum Tech.","PTDD03N2-2R5M160",4,16,"V","-","-","150(80ﾟC)","-","-",550,2.5,20,20,1.5,5,"-","-","-","-","-",5,"-","-",0.5,"-","-","-","-","-","-","-"]
["Murata","PTGL05AR1R0M1B51A0",5,16,"VDC",470,370,252,880,1040,1095,1,20,20,2,6,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL5SAR1R0M1B51A0",5,16,"VDC",470,370,252,880,1040,1095,1,20,20,2,6,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL05AR1R0M1B51B0",5,16,"VDC",470,370,252,880,1040,1095,1,20,20,2,6,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL5SAR1R0M1B51B0",5,16,"VDC",470,370,252,880,1040,1095,1,20,20,2,6,null,null,3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL5SAR1R0M1B53A0",5,16,"VDC",470,370,252,880,1040,1095,1,20,20,2,6,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL5SAR1R0M1B53B0",5,16,"VDC",470,370,252,880,1040,1095,1,20,20,2,6,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59975C0120A070",5,30,"Vrms.",450,337.5,247.50000000000003,900,1080,"-",1.8,25,25,3,9,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,85,-40,125,"-"]
["Thinking","PPL081R8*A224",5,24,"Vrms.",450,"-","-",900,"-","-",1.8,"-","-",3,"7.5to10","-","-","1.5to3.5","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL09H541D*E",5,30,"Vrms.",540,432,334.8,810,955.8,1036.8,1.9,20,20,6,8.5,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL06AR0R8M1B51A0",6,16,"VDC",505,400,"-",955,1120,"-",0.8,20,20,3,6.5,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL6SAR0R8M1B51A0",6,16,"VDC","-",400,"-","-",1120,"-",0.8,20,20,3,6.5,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,"-","-","-"]
["Murata","PTGL06AR0R8M1B51B0",6,16,"VDC",505,400,"-",955,1120,"-",0.8,20,20,3,6.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL6SAR0R8M1B51B0",6,16,"VDC","-",400,274,"-",1120,1193,0.8,20,20,3,6.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,"-","-","-"]
["Murata","PTGL6SAR0R8M1B54B1",6,16,"VDC",505,400,274,955,1120,1193,0.8,20,20,3,6.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,90,"Special specification type"]
["TDK/EPCOS","B59975C0160A070",6,20,"Vrms.",550,440,368.5,1100,1265,"-",1.8,25,25,3,9,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,85,-40,125,"-"]
["Thinking","PPL081R8*A224",6,24,"Vrms.",450,"-","-",900,"-","-",1.8,"-","-",3,"7.5to10","-","-","1.5to3.5","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL09H541D*E",6,30,"Vrms.",540,432,334.8,810,955.8,1036.8,1.9,20,20,6,8.5,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL07BA0R9M1B51A0",7,16,"Vrms.","-",405,"-","-",1200,"-",0.9,20,20,3,7.4,"-","-",4,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL07BA0R9M1B51B0",7,16,"Vrms.","-",405,"-","-",1200,"-",0.9,20,20,3,7.4,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59975C0160A070",7,20,"Vrms.",550,440,368.5,1100,1265,"-",1.8,25,25,3,9,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,85,-40,125,"-"]
["Thinking","PPL101R2*A212",7,12,"Vrms.",600,"-","-",1200,"-","-",1.2,"-","-",4.3,"9.5to12","-","-","1.5to3.5","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Nichicon","ZPC13CE1R5K",7,16,"V","-",410,"-","-",1030,"-",1.5,20,20,2.1,7,"-","-",3,"-","-",5,"-","-",0.5,"-","-","-","-","-","-","-"]
["Murata","PTGL7SARR47M1N51A0",8,16,"VDC","-",480,350,"-",1330,1420,0.47,20,20,5,7.5,"-","-",3.5,"-","-",5,0.3,0.8,0.5,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL7SARR47M1N51B0",8,16,"VDC","-",480,350,"-",1330,1420,0.47,20,20,5,7.5,"-","-",3.5,"-","-",5,1.5,1.5,0.5,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL07ARR47M1B51A0",8,16,"VDC",705,560,"-",1310,1570,"-",0.47,20,20,5,7.5,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL7SARR47M1B51A0",8,16,"VDC",705,560,"-",1310,1570,"-",0.47,20,20,5,7.5,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL07ARR47M1B51B0",8,16,"VDC",705,560,"-",1310,1570,"-",0.47,20,20,5,7.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL7SARR47M1B51B0",8,16,"VDC",705,560,"-",1310,1570,"-",0.47,20,20,5,7.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"-"]
["TDK/EPCOS","B59965C0160A070",8,20,"Vrms.",700,560,469,1450,1667.4999999999998,"-",1.2,25,25,4.3,11,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,85,-40,125,"-"]
["Thinking","PPL101R3*A424",8,24,"Vrms.",700,"-","-",1400,"-","-",1.3,"-","-",8,"9.5to12","-","-","2.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL13H831D*E",8,30,"Vrms.",830,664,514.6,1245,1469.1,1593.6000000000001,1.1000000000000001,20,20,10,12.5,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL12AR1R2M2A64B0",9,16,"Vrms.","-",570,"-","-",1450,"-",1.2,20,20,4,12,"-","-",4,"-","-",6.4,1.5,1.5,0.5,0.05,0.05,"-","-","-","-","Special specification type"]
["Murata","PTGL12AR1R2M2B51A0",9,16,"Vrms.","-",570,"-","-",1450,"-",1.2,20,20,4,12,"-","-",4,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL12AR1R2M2B51B0",9,16,"Vrms.","-",570,"-","-",1450,"-",1.2,20,20,4,12,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59965C0160A070",9,20,"Vrms.",700,560,469,1450,1667.4999999999998,"-",1.2,25,25,4.3,11,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,85,-40,125,"-"]
["Thinking","PPL101R3*A424",9,24,"Vrms.",700,"-","-",1400,"-","-",1.3,"-","-",8,"9.5to12","-","-","2.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL11H701D*E",9,30,"Vrms.",700,560,434,1050,1239,1344,1.3,20,20,8,10.5,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL09BA0R5M1B51A0",10,16,"Vrms.","-",600,"-","-",1750,"-",0.5,20,20,5,9.5,"-","-",4,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL09BA0R5M1B51B0",10,16,"Vrms.","-",600,"-","-",1750,"-",0.5,20,20,5,9.5,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["Nichicon","ZPC17CE0R8K",10,16,"V","-",600,"-","-",1490,"-",0.8,20,20,4.0999999999999996,8.8000000000000007,"-","-",3,"-","-",5,"-","-",0.6,"-","-","-","-","-","-","-"]
["Murata","PTGL09BA0R5M1P51B0",11,16,"Vrms.","-","-",315,"-","-",1350,0.5,20,20,5,9.5,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","Special specification type"]
["TDK/EPCOS","B59965C0120A070",11,30,"Vrms.",600,450,330,1200,1440,"-",1.2,25,25,4.3,11,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,85,-40,125,"-"]
["Murata","PTGL13AR0R9M1N04B0",12,16,"Vrms.","-","-","-","-","-","-",0.9,20,20,"-","-","-","-","-","-","-","-","-","-",0.5,0.05,0.05,-10,60,"-","-","Special specification type"]
["Murata","PTGL13AR1R0M1C01B0",12,16,"Vrms.","-",550,"-","-",1550,"-",1,20,20,5,13.5,"-","-",4,"-","-",10,1.5,1.5,0.65,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL13AR1R0M1C04B0",12,16,"Vrms.","-",630,"-","-",1730,"-",1,20,20,5,14,"-","-",4,"-","-",10,1.5,1.5,0.65,0.05,0.05,-10,60,"-","-","Special specification type"]
["TDK/EPCOS","B59955C0120A070",12,30,"Vrms.",850,637.5,467.50000000000006,1700,2040,"-",0.8,25,25,5.5,13.5,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,85,-40,125,"-"]
["Thinking","PPL140R5*A212",12,12,"Vrms.",870,"-","-",2450,"-","-",0.5,"-","-",5,"13.5to16","-","-","1.5to3.5","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Murata","PTGL09ARR33M1B51A0",13,16,"VDC",875,680,"-",1625,1900,"-",0.33,20,20,7,9,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL9SARR33M1B51A0",13,16,"VDC","-",680,466,"-",1900,2026,0.33,20,20,7,9,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,"-","-","-"]
["Murata","PTGL09ARR33M1B51B0",13,16,"VDC",875,680,"-",1625,1900,"-",0.33,20,20,7,9,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL9SARR33M1B51B0",13,16,"VDC","-",680,466,"-",1900,2026,0.33,20,20,7,9,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,"-","-","-"]
["Murata","PTGL9SARR33M1B54B1",13,16,"VDC","-",680,466,"-",1900,2026,0.33,20,20,7,9,"-","-",3.5,"-","-",5,1,1,0.6,0.05,0.05,-30,85,-40,90,"Special specification type"]
["TDK/EPCOS","B59955C0120A070",13,30,"Vrms.",850,637.5,467.50000000000006,1700,2040,"-",0.8,25,25,5.5,13.5,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,85,-40,125,"-"]
["Thinking","PPL121R1*A424",13,24,"Vrms.",830,"-","-",1660,"-","-",1.1000000000000001,"-","-",10,"11.5to14","-","-","2.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL13H921D*E",13,30,"Vrms.",920,736,570.4,1380,1628.3999999999999,1766.4,0.9,20,20,11,12.5,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL10ARR27M1B51A0",14,16,"VDC",1025,800,"-",1900,2250,"-",0.27,20,20,8,10.1,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGLASARR27M1B51A0",14,16,"VDC",1025,800,"-",1900,2250,"-",0.27,20,20,8,10.1,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,"-","-","-"]
["Murata","PTGL10ARR27M1B51B0",14,16,"VDC",1025,800,"-",1900,2250,"-",0.27,20,20,8,10.1,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGLASARR27M1B51B0",14,16,"VDC",1025,800,"-",1900,2250,"-",0.27,20,20,8,10.1,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,"-","-","-"]
["Murata","PTGL10ARR27M1B51B1",14,16,"VDC",1025,800,"-",1900,2250,"-",0.27,20,20,8,10.1,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,"-","-","Special specification type"]
["Murata","PTGL12BA0R3H1B51A0",14,16,"Vrms.","-",800,"-","-",2400,"-",0.3,25,25,7,12,"-","-",4,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL12BA0R3H1B51B0",14,16,"Vrms.","-",800,"-","-",2400,"-",0.3,25,25,7,12,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59955C0160A070",14,20,"Vrms.",950,760,636.5,1900,2185,"-",0.8,25,25,5.5,13.5,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,85,-40,125,"-"]
["Thinking","PPL120R5*A224",14,24,"Vrms.",1000,"-","-",2000,"-","-",0.5,"-","-",6.5,"11.5to14","-","-","1.5to3.5","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL17H112DBE",14,30,"Vrms.",1170,936,725.4,1755,2070.9,2246.4,0.7,20,20,13.5,16.5,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"Bulk"]
["Nichicon","ZPC1MCC0R3K",14,16,"V","-",1030,"-","-",2580,"-",0.3,20,20,7,11.9,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-","-","-","-","-","-"]
["Murata","PTGL12AR0R2M1B51A0",15,16,"VDC",1300,1000,"-",2410,2800,"-",0.2,20,20,9,11.3,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGLCSAR0R2M1B51A0",15,16,"VDC",1300,1000,692,2410,2800,"-",0.2,20,20,9,11.3,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL12AR0R2M1B51B0",15,16,"VDC",1300,1000,"-",2410,2800,"-",0.2,20,20,9,11.3,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGLCSAR0R2M1B51B0",15,16,"VDC",1300,1000,692,2410,2800,"-",0.2,20,20,9,11.3,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGLCSAR0R2M1B54B1",15,16,"VDC",1300,1000,692,2410,2800,"-",0.2,20,20,9,11.3,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","Special specification type"]
["Murata","PTGL14BA0R2H1B71B0",15,16,"Vrms.","-",1050,"-","-",3200,"-",0.2,25,25,8,15,"-","-",4,"-","-",5,1.5,1.5,7.5,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL14BA0R2H1B74B0",15,16,"Vrms.","-",1050,"-","-",3200,"-",0.2,25,25,8,15,"-","-",4,"-","-",5,1.5,1.5,7.5,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59945C0120A070",15,30,"Vrms.",1300,975,715.00000000000011,2600,3120,"-",0.45,25,25,8,17.5,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,85,-40,125,"-"]
["Thinking","PPL160R5*A212",15,12,"Vrms.",1300,"-","-",2600,"-","-",0.5,"-","-",8,"15to17.5","-","-","3to5","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL17H132DBE",15,30,"Vrms.",1390,1112,861.8,2085,2460.2999999999997,2668.8,0.5,20,20,16,16.5,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"Bulk"]
["Murata","PTGL14ARR15M1B51B0",16,16,"Vrms.",1545,1200,"-",2855,3360,"-",0.15,20,20,10,13.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGLESARR15M1B51B0",16,16,"Vrms.",1545,1200,820,2855,3360,3561,0.15,20,20,10,13.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,"-","-","-"]
["Murata","PTGLESARR15M1B51A0",16,16,"Vrms.",1545,1200,820,2855,3360,3561,0.15,20,20,10,13.5,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,"-","-","-"]
["TDK/EPCOS","B59945C0160A070",16,20,"Vrms.",1500,1200,1005.0000000000001,3050,3507.4999999999995,"-",0.45,25,25,8,17.5,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,85,-40,125,"-"]
["Thinking","PPL160R5*A424",16,24,"Vrms.",1390,"-","-",2780,"-","-",0.5,"-","-",16,"15to17.5","-","-","2.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL17H132DBE",16,30,"Vrms.",1390,1112,861.8,2085,2460.2999999999997,2668.8,0.5,20,20,16,16.5,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"Bulk"]
["Murata","PTGL07BD6R8N2B51A0",17,24,"Vrms.",139,90,"-",296,370,"-",6.8,30,30,2,7.4,"-","-",4,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL07BD6R8N2B51B0",17,24,"Vrms.",139,90,"-",296,370,"-",6.8,30,30,2,7.4,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59960C0080A070",17,80,"Vrms.",130,74.099999999999994,"-",265,371,"-",5.6,25,25,4.3,9,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,85,-40,125,"-"]
["Thinking","PPL03130*A224",17,24,"Vrms.",120,"-","-",240,"-","-",13,"-","-",0.7,"2.5to4.0","-","-","1.5to3.5","-","-",5,1,1,0.5,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL05H131E*E",17,60,"Vrms.",130,104,80.599999999999994,195,230.1,249.6,25,20,20,1.2,5,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL09BD4R7N2B51A0",18,24,"Vrms.",216,120,"-",398,500,"-",4.7,30,30,2,9.5,"-","-",4,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL09BD4R7N2B51B0",18,24,"Vrms.",216,120,"-",398,500,"-",4.7,30,30,2,9.5,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59960C0130A070",18,80,"Vrms.",250,195,155,380,456,"-",8,20,20,3,11,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,125,-40,125,"-"]
["Thinking","PPL088R0*A363",18,63,"Vrms.",250,"-","-",380,"-","-",8,"-","-",3,"7.5to10","-","-","2.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL05H271D*E",18,30,"Vrms.",270,216,167.4,405,477.9,518.4,6,20,20,2.5,5,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL09BD3R3N2B51A0",19,24,"VDC",248,140,"-",461,580,"-",3.3,30,30,2,9.5,"-","-",4,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL09BD3R3N2B51B0",19,24,"VDC",248,140,"-",461,580,"-",3.3,30,30,2,9.5,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59960C0130A070",19,80,"Vrms.",250,195,155,380,456,"-",8,20,20,3,11,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,125,-40,125,"-"]
["Thinking","PPL088R0*A363",19,63,"Vrms.",250,"-","-",380,"-","-",8,"-","-",3,"7.5to10","-","-","2.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL05H271D*E",19,30,"Vrms.",270,216,167.4,405,477.9,518.4,6,20,20,2.5,5,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL09AR2R7M2B51A0",20,28,"VDC","-",300,"-","-",850,"-",2.7,20,20,3,9.5,"-","-",4,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,"-","-","-"]
["Murata","PTGL09AR2R7M2B51B0",20,28,"VDC","-",300,"-","-",850,"-",2.7,20,20,3,9.5,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,"-","-","-"]
["TDK/EPCOS","B59975C0120A070",20,30,"Vrms.",450,337.5,247.50000000000003,900,1080,"-",1.8,25,25,3,9,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,85,-40,125,"-"]
["Thinking","PPL143R3*A224",20,24,"Vrms.",420,"-","-",980,"-","-",3.3,"-","-",5,"13.5to16","-","-","1.5to3.5","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL07H411D*E",20,30,"Vrms.",410,328,254.2,615,725.69999999999993,787.2,3,20,20,4.5,7,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL04AS100K2N51A0",21,30,"Vrms.",154,122,"-",205,240,"-",10,10,10,1.5,4.5,"-","-",3.5,"-","-",5,0.3,0.8,0.5,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL4SAS100K2N51A0",21,30,"Vrms.",154,"-",92,205,240,"-",10,10,10,1.5,4.5,"-","-",3.5,"-","-",5,0.3,0.8,0.5,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL04AS100K2N51B0",21,30,"Vrms.",154,122,92,205,240,"-",10,10,10,1.5,4.5,"-","-",3.5,"-","-",5,1.5,1.5,0.5,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL4SAS100K2N51B0",21,30,"Vrms.",154,"-",92,205,240,"-",10,10,10,1.5,4.5,"-","-",3.5,"-","-",5,1.5,1.5,0.5,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL04AS100K2N51B1",21,30,"Vrms.",154,122,"-",205,240,"-",10,10,10,1.5,4.5,"-","-",3.5,"-","-",5,1.5,1.5,0.5,0.05,0.05,-30,85,-40,125,"Special specification type"]
["Murata","PTGL04AS100K2N52AL",21,30,"Vrms.",154,"-","-",205,"-","-",10,10,10,1.5,4.5,"-","-",3.5,"-","-",5,0.3,0.8,0.5,0.05,0.05,"-","-","-","-","Special specification type"]
["Murata","PTGL04AS100M2N51A0",21,30,"Vrms.","-","-","-","-","-","-",10,20,20,1.5,4.5,"-","-",3.5,"-","-",5,0.3,0.8,0.5,0.05,0.05,"-","-","-","-","Special specification type"]
["Murata","PTGL04AS100M2N51B0",21,30,"Vrms.","-","-","-","-","-","-",10,20,20,1.5,4.5,"-","-",3.5,"-","-",5,0.3,0.8,0.5,0.05,0.05,"-","-","-","-","Special specification type"]
["TDK/EPCOS","B59995C0120A070",21,30,"Vrms.",120,90,66,240,288,"-",13,25,25,0.7,4,"-","-",3.5,"-","-",5,"-","-",0.5,"-","-",-40,85,-40,125,"-"]
["Vishay","PTCCL05H131F*E",21,145,"Vrms.",130,104,80.599999999999994,195,230.1,249.6,28,20,20,0.6,5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL05AS3R9K2B51A0",22,30,"Vrms.",340,269,"-",452,530,"-",3.9,10,10,3.5,5.5,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL5SAS3R9K2B51A0",22,30,"Vrms.",340,"-",204,452,530,"-",3.9,10,10,3.5,5.5,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL05AS3R9K2B51B0",22,30,"Vrms.",340,269,"-",452,530,"-",3.9,10,10,3.5,5.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL5SAS3R9K2B51B0",22,30,"Vrms.",340,"-",204,452,530,"-",3.9,10,10,3.5,5.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL05AS3R9K2B51B2",22,30,"Vrms.",340,269,"-",452,530,"-",3.9,10,10,3.5,5.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Thinking","PPL103R9*A224",22,24,"Vrms.",340,"-","-",800,"-","-",3.9,"-","-",4.3,"9.5to12","-","-","1.5to3.5","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL07H321D*E",22,30,"Vrms.",320,256,198.4,480,566.4,614.4,5,20,20,3.5,7,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL04AR130H2B51A0",23,30,"Vrms.",180,145,"-",350,400,"-",13,25,25,1,5.5,"-","-",4,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-30,85,"-"]
["Murata","PTGL04AR130H2B51B0",23,30,"Vrms.",180,145,"-",350,400,"-",13,25,25,1,5.5,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-30,85,"-"]
["TDK/EPCOS","B59995C0120A070",23,30,"Vrms.",120,90,66,240,288,"-",13,25,25,0.7,4,"-","-",3.5,"-","-",5,"-","-",0.5,"-","-",-40,85,-40,125,"-"]
["Thinking","PPL08180*A248",23,48,"Vrms.",195,"-","-",390,"-","-",18,"-","-",1.6,"7.5to10","-","-","2.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL05H181D*E",23,30,"Vrms.",180,144,111.6,270,318.59999999999997,345.6,13,20,20,1.7,5,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL04AS100K2B51A0",24,30,"Vrms.",212,167,"-",282,330,"-",10,10,10,2,4.5,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL4SAS100K2B51A0",24,30,"Vrms.",212,"-",127,282,330,"-",10,10,10,2,4.5,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL04AS100K2B51B0",24,30,"Vrms.",212,167,"-",282,330,"-",10,10,10,2,4.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL4SAS100K2B51B0",24,30,"Vrms.",212,"-",127,282,330,"-",10,10,10,2,4.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL4SAS100K2B51B1",24,30,"Vrms.",212,"-",127,282,330,"-",10,10,10,2,4.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL04AS100K2B52AL",24,30,"Vrms.",212,167,"-",282,330,"-",10,10,10,2,4.5,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Vishay","PTCCL05H181D*E",24,30,"Vrms.",180,144,111.6,270,318.59999999999997,345.6,13,20,20,1.7,5,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL07AR4R6H2B51A0",25,30,"Vrms.",340,250,"-",610,700,"-",4.5999999999999996,25,25,1,7.4,"-","-",4,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL07AR4R6H2B51B0",25,30,"Vrms.",340,250,"-",610,700,"-",4.5999999999999996,25,25,1,7.4,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59975C0120A070",25,30,"Vrms.",450,337.5,247.50000000000003,900,1080,"-",1.8,25,25,3,9,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,85,-40,125,"-"]
["Thinking","PPL126R5*A248",25,48,"Vrms.",350,"-","-",700,"-","-",6.5,"-","-",4,"11.5to14","-","-","2.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL07H411D*E",25,30,"Vrms.",410,328,254.2,615,725.69999999999993,787.2,3,20,20,4.5,7,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL07AS2R7K2B51A0",26,30,"Vrms.",425,336,255,565,663,"-",2.7,10,10,4.5,7.3,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL7SAS2R7K2B51A0",26,30,"Vrms.",425,"-",255,565,"-","-",2.7,10,10,4.5,7.3,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL07AS2R7K2B51B0",26,30,"Vrms.",425,336,255,565,663,"-",2.7,10,10,4.5,7.3,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL7SAS2R7K2B51B0",26,30,"Vrms.",425,"-",255,565,"-","-",2.7,10,10,4.5,7.3,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-40,125,-40,125,"-"]
["TDK/EPCOS","B59975C0120A070",26,30,"Vrms.",450,337.5,247.50000000000003,900,1080,"-",1.8,25,25,3,9,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,85,-40,125,"-"]
["Vishay","PTCCL07H411D*E",26,30,"Vrms.",410,328,254.2,615,725.69999999999993,787.2,3,20,20,4.5,7,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL09AR1R8H2B51A0",27,30,"Vrms.",510,410,"-",970,1120,"-",1.8,25,25,3,9.5,"-","-",4,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL09AR1R8H2B51B0",27,30,"Vrms.",510,410,"-",970,1120,"-",1.8,25,25,3,9.5,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL09AR1R8H2B51B9",27,30,"Vrms.",510,410,"-",970,1120,"-",1.8,25,25,3,9.5,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","Special specification type"]
["TDK/EPCOS","B59975C0120A070",27,30,"Vrms.",450,337.5,247.50000000000003,900,1080,"-",1.8,25,25,3,9,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,85,-40,125,"-"]
["Thinking","PPL163R8*A248",27,48,"Vrms.",505,"-","-",1010,"-","-",3.8,"-","-",7.3,"15to17.5","-","-","2.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL11H611D*E",27,30,"Vrms.",610,488,378.2,915,1079.7,1171.2,1.7,20,20,7,10.5,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL07AS1R8K2B51A0",28,30,"Vrms.",532,420,319,708,829,"-",1.8,10,10,5,7.3,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL7SAS1R8K2B51A0",28,30,"Vrms.",532,"-",319,708,829,"-",1.8,10,10,5,7.3,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL07AS1R8K2B51B0",28,30,"Vrms.",532,420,319,708,829,"-",1.8,10,10,5,7.3,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL7SAS1R8K2B51B0",28,30,"Vrms.",532,"-",319,708,829,"-",1.8,10,10,5,7.3,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Thinking","PPL081R9*A424",28,24,"Vrms.",540,"-","-",1080,"-","-",1.9,"-","-",6,"7.5to10","-","-","2.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL09H541D*E",28,30,"Vrms.",540,432,334.8,810,955.8,1036.8,1.9,20,20,6,8.5,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL12AR1R2H2B51B0",29,30,"Vrms.",645,520,"-",1225,1420,"-",1.2,25,25,4.3,12,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,"-","-","-"]
["TDK/EPCOS","B59965C0120A070",29,30,"Vrms.",600,450,330,1200,1440,"-",1.2,25,25,4.3,11,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,85,-40,125,"-"]
["Thinking","PPL202R2*A248",29,48,"Vrms.",725,"-","-",1450,"-","-",2.2000000000000002,"-","-",14,"19to22","-","-","2.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL11H701D*E",29,30,"Vrms.",700,560,434,1050,1239,1344,1.3,20,20,8,10.5,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL09AS1R2K2B51A0",30,30,"Vrms.",704,556,"-",936,1097,"-",1.2,10,10,6,9.3000000000000007,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL9SAS1R2K2B51A0",30,30,"Vrms.",704,"-",422,936,1097,"-",1.2,10,10,6,9.3000000000000007,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL09AS1R2K2B51B0",30,30,"Vrms.",704,556,"-",936,1097,"-",1.2,10,10,6,9.3000000000000007,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL9SAS1R2K2B51B0",30,30,"Vrms.",704,"-",422,936,1097,"-",1.2,10,10,6,9.3000000000000007,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-40,125,-40,125,"-"]
["TDK/EPCOS","B59965C0120A070",30,30,"Vrms.",600,450,330,1200,1440,"-",1.2,25,25,4.3,11,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,85,-40,125,"-"]
["Thinking","PPL101R7*A424",30,24,"Vrms.",610,"-","-",1220,"-","-",1.7,"-","-",7,"9.5to12","-","-","2.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL11H701D*E",30,30,"Vrms.",700,560,434,1050,1239,1344,1.3,20,20,8,10.5,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL12AS0R8K2B51A0",31,30,"Vrms.",867,685,520,1153,1352,"-",0.8,10,10,7,11.5,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGLCSAS0R8K2B51A0",31,30,"Vrms.",867,"-",520,1153,"-","-",0.8,10,10,7,11.5,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL12AS0R8K2B51B0",31,30,"Vrms.",867,685,520,1153,1352,"-",0.8,10,10,7,11.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGLCSAS0R8K2B51B0",31,30,"Vrms.",867,"-",520,1153,"-","-",0.8,10,10,7,11.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Thinking","PPL120R9*A424",31,24,"Vrms.",920,"-","-",1840,"-","-",0.9,"-","-",11,"11.5to14","-","-","2.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL13H831D*E",31,30,"Vrms.",830,664,514.6,1245,1469.1,1593.6000000000001,1.1000000000000001,20,20,10,12.5,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL13AR0R8H2B71B0",32,30,"Vrms.",870,680,"-",1600,1900,"-",0.8,25,25,5.5,13.5,"-","-",4,"-","-",7.5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59955C0120A070",32,30,"Vrms.",850,637.5,467.50000000000006,1700,2040,"-",0.8,25,25,5.5,13.5,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,85,-40,125,"-"]
["Thinking","PPL201R6*A248",32,48,"Vrms.",870,"-","-",1750,"-","-",1.6,"-","-",18,"19to22","-","-","2.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL13H921D*E",32,30,"Vrms.",920,736,570.4,1380,1628.3999999999999,1766.4,0.9,20,20,11,12.5,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL07BD330N3B51A0",33,32,"Vrms.",60,40,"-",135,170,"-",33,30,30,1.5,7.4,"-","-",4,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL07BD330N3B51B0",33,32,"Vrms.",60,40,"-",135,170,"-",33,30,30,1.5,7.4,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL07BD330N3B51B9",33,32,"Vrms.",60,40,"-",135,170,"-",33,30,30,1.5,7.4,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","Special specification type"]
["TDK/EPCOS","B59875C0120A570",33,265,"Vrms.",80,60,44,120,144,"-",39,20,20,1,9,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Thinking","PPL06150*P842",33,42,"Vrms.",60,"-","-",230,"-","-",15,"-","-",1.5,"5.5to8","-","-","2.0to4.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL05H940E*E",33,60,"Vrms.",94,75.2,58.28,145,171.1,185.6,50,20,20,0.8,5,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL07BD220N3B51A0",34,32,"Vrms.",75,45,"-",160,200,"-",22,30,30,1.5,7.4,"-","-",4,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL07BD220N3B51B0",34,32,"Vrms.",75,45,"-",160,200,"-",22,30,30,1.5,7.4,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL07BD200Q3B31A9",34,32,"Vrms.","-","-","-","-","-","-",20,40,40,1.5,7.4,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","Special specification type"]
["TDK/EPCOS","B59970C0080A070",34,80,"Vrms.",90,51.3,"-",190,266,"-",9.4,25,25,3,6.5,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,85,-40,125,"-"]
["Thinking","PPL04620*A363",34,63,"Vrms.",85,"-","-",130,"-","-",62,"-","-",0.7,"4.0to6.5","-","-","2.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Murata","PTGL07BD150N3B51A0",35,32,"Vrms.",100,60,"-",195,240,"-",15,30,30,1.5,7.4,"-","-",4,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL07BD150N3B51B0",35,32,"Vrms.",100,60,"-",195,240,"-",15,30,30,1.5,7.4,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59970C0080A070",35,80,"Vrms.",90,51.3,"-",190,266,"-",9.4,25,25,3,6.5,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,85,-40,125,"-"]
["Vishay","PTCCL05H131E*E",35,60,"Vrms.",130,104,80.599999999999994,195,230.1,249.6,25,20,20,1.2,5,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL07AR4R7M2P51A0",36,32,"Vrms.","-",150,"-","-",390,"-",4.7,20,20,2,7.4,"-","-",4,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL07AR4R7M2P51B0",36,32,"Vrms.","-",150,"-","-",390,"-",4.7,20,20,2,7.4,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59985C0120A070",36,30,"Vrms.",250,187.5,137.5,500,600,"-",4.5999999999999996,25,25,1,6.5,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,85,-40,125,"-"]
["Thinking","PPL089R1*A263",36,63,"Vrms.",160,"-","-",480,"-","-",9.1,"-","-",3,"7.5to10","-","-","2.0to4.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL05H181D*E",36,30,"Vrms.",180,144,111.6,270,318.59999999999997,345.6,13,20,20,1.7,5,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL09AR3R9M3P51A0",37,32,"Vrms.","-",190,"-","-",520,"-",3.9,20,20,2,9.5,"-","-",4,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,"-","-","-"]
["Murata","PTGL09AR3R9M3P51B0",37,32,"Vrms.","-",190,"-","-",520,"-",3.9,20,20,2,9.5,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,"-","-","-"]
["TDK/EPCOS","B59985C0120A070",37,30,"Vrms.",250,187.5,137.5,500,600,"-",4.5999999999999996,25,25,1,6.5,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,85,-40,125,"-"]
["Murata","PTGL09AR3R9M3B51A0",38,32,"Vrms.","-",270,"-","-",740,"-",3.9,20,20,2,9.5,"-","-",4,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL09AR3R9M3B51B0",38,32,"Vrms.","-",270,"-","-",740,"-",3.9,20,20,2,9.5,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59950C0130A070",38,80,"Vrms.",320,249.60000000000002,198.4,500,600,"-",4.9000000000000004,20,20,4.3,13.5,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,125,-40,125,"-"]
["Vishay","PTCCL11H361F*E",38,145,"Vrms.",360,288,223.2,540,637.19999999999993,691.2,5.3,20,20,3.5,10.5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Nichicon","ZPC2ECE3R3K",38,35,"V","-",310,"-","-",790,"-",3.3,20,20,2.2000000000000002,11.9,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-","-","-","-","-","-"]
["Murata","PTGL07AR6R8M2B51A0",39,35,"Vrms.","-",220,"-","-",580,"-",6.8,20,20,1.5,7.4,"-","-",4,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL07AR6R8M2B51B0",39,35,"Vrms.","-",220,"-","-",580,"-",6.8,20,20,1.5,7.4,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59950C0130A070",39,80,"Vrms.",320,249.60000000000002,198.4,500,600,"-",4.9000000000000004,20,20,4.3,13.5,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,125,-40,125,"-"]
["Murata","PTGL04AS100K3B51A0",40,51,"Vrms.",213,168,128,283,332,"-",10,10,10,1,4.5,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL4SAS100K3B51A0",40,51,"Vrms.",213,"-",128,283,"-","-",10,10,10,1,4.5,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL04AS100K3B51B0",40,51,"Vrms.",213,168,128,283,332,"-",10,10,10,1,4.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL4SAS100K3B51B0",40,51,"Vrms.",213,"-",128,283,"-","-",10,10,10,1,4.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Vishay","PTCCL07H211F*E",40,145,"Vrms.",210,168,130.19999999999999,315,371.7,403.2,12,20,20,1.4,7,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL05AS6R8K3B51A0",41,51,"Vrms.",249,197,149,331,388,"-",6.8,10,10,1.5,5.5,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-30,125,"-"]
["Murata","PTGL5SAS6R8K3B51A0",41,51,"Vrms.",249,"-",149,331,338,"-",6.8,10,10,1.5,5.5,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL05AS6R8K3B51B0",41,51,"Vrms.",249,197,149,331,388,"-",6.8,10,10,1.5,5.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-30,125,"-"]
["Murata","PTGL5SAS6R8K3B51B0",41,51,"Vrms.",249,"-",149,331,338,"-",6.8,10,10,1.5,5.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-40,125,-40,125,"-"]
["TDK/EPCOS","B59960C0130A070",41,80,"Vrms.",250,195,155,380,456,"-",8,20,20,3,11,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,125,-40,125,"-"]
["Vishay","PTCCL09H251F*E",41,145,"Vrms.",250,200,155,375,442.5,480,9.4,20,20,2,8.5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL07AS3R3K3B51A0",42,51,"Vrms.",389,307,"-",517,606,"-",3.3,10,10,3,7.3,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL7SAS3R3K3B51A0",42,51,"Vrms.",389,"-",233,517,606,"-",3.3,10,10,3,7.3,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL07AS3R3K3B51B0",42,51,"Vrms.",389,307,"-",517,606,"-",3.3,10,10,3,7.3,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL7SAS3R3K3B51B0",42,51,"Vrms.",389,"-",233,517,606,"-",3.3,10,10,3,7.3,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL07AS3R3K3B52AL",42,51,"Vrms.",389,307,"-",517,606,"-",3.3,10,10,3,7.3,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"Special specification type"]
["TDK/EPCOS","B59950C0130A070",42,80,"Vrms.",320,249.60000000000002,198.4,500,600,"-",4.9000000000000004,20,20,4.3,13.5,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,125,-40,125,"-"]
["Vishay","PTCCL11H361F*E",42,145,"Vrms.",360,288,223.2,540,637.19999999999993,691.2,5.3,20,20,3.5,10.5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL09AS2R2K3B51A0",43,51,"Vrms.",522,412,"-",694,814,"-",2.2000000000000002,10,10,4,9.3000000000000007,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL9SAS2R2K3B51A0",43,51,"Vrms.",522,"-",313,694,814,"-",2.2000000000000002,10,10,4,9.3000000000000007,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,"-","-","-","-","-"]
["Murata","PTGL09AS2R2K3B51B0",43,51,"Vrms.",522,412,"-",694,814,"-",2.2000000000000002,10,10,4,9.3000000000000007,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL9SAS2R2K3B51B0",43,51,"Vrms.",522,"-",313,694,814,"-",2.2000000000000002,10,10,4,9.3000000000000007,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-40,125,"-","-","-"]
["Murata","PTGL09AS2R2K3B52AL",43,51,"Vrms.",522,412,"-",694,814,"-",2.2000000000000002,10,10,4,9.3000000000000007,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,"-","-","-","-","Special specification type"]
["Thinking","PPL123R3*A363",43,63,"Vrms.",450,"-","-",690,"-","-",3.3,"-","-",5.5,"11.5to14","-","-","2.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL13H451F*E",43,145,"Vrms.",450,360,279,675,796.5,864,3.8,20,20,5,12.5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL12AS1R2K3B51A0",44,51,"VDC",749,592,"-",996,1168,"-",1.2,10,10,5,11.5,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGLCSAS1R2K3B51A0",44,51,"VDC",749,"-",449,996,1168,"-",1.2,10,10,5,11.5,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,125,-40,125,"-"]
["Murata","PTGL12AS1R2K3B51B0",44,51,"VDC",749,592,"-",996,1168,"-",1.2,10,10,5,11.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGLCSAS1R2K3B51B0",44,51,"VDC",749,"-",449,996,1168,"-",1.2,10,10,5,11.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,125,-40,125,"-"]
["Murata","PTGLCSAS1R2K3B51B1",44,51,"VDC",749,"-",449,996,1168,"-",1.2,10,10,5,11.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,125,-40,125,"Special specification type"]
["TDK/EPCOS","B59930C0130A070",44,80,"Vrms.",700,546,434,1100,1320,"-",2.2000000000000002,20,20,8,17.5,"-","-",3.5,"-","-",5,"-","-",0.8,"-","-",-40,125,-40,125,"-"]
["Thinking","PPL162R2*A363",44,63,"Vrms.",700,"-","-",1100,"-","-",2.2000000000000002,"-","-",8,"15to17.5","-","-","2.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL17H711FBE",44,145,"Vrms.",710,568,440.2,1065,1256.7,1363.2,2.1,20,20,8.5,16.5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"Bulk"]
["Murata","PTGL07AR680M3B51A0",45,56,"Vrms.","-",75,"-","-",190,"-",68,20,20,0.5,7.4,"-","-",4,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL07AR680M3B51B0",45,56,"Vrms.","-",75,"-","-",190,"-",68,20,20,0.5,7.4,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59870C0130A070",45,265,"Vrms.",100,80,67,150,180,"-",50,20,20,0.4,9,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Thinking","PPL05240*A263",45,63,"Vrms.",90,"-","-",270,"-","-",24,"-","-",1,"4.5to7","-","-","2.0to4.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Murata","PTGL07AR220M3N54B0",46,56,"Vrms.","-",85,"-","-",200,"-",22,20,20,0.8,7.4,"-","-",5,"-","-",5,1.5,1.5,0.5,0.05,0.05,-10,60,"-","-","-"]
["Vishay","PTCCL05H131E*E",46,60,"Vrms.",130,104,80.599999999999994,195,230.1,249.6,25,20,20,1.2,5,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL07AR470M3B51A0",47,56,"Vrms.","-",85,"-","-",225,"-",47,20,20,0.5,7.4,"-","-",4,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL07AR470M3B51B0",47,56,"Vrms.","-",85,"-","-",225,"-",47,20,20,0.5,7.4,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL07AR470M3B54B0",47,56,"Vrms.","-",85,"-","-",225,"-",47,20,20,0.5,7.4,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59870C0130A070",47,265,"Vrms.",100,80,67,150,180,"-",50,20,20,0.4,9,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Vishay","PTCCL05H111F*E",47,145,"Vrms.",110,88,68.2,165,194.7,211.20000000000002,40,20,20,0.5,5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL07AR220M3P51A0",48,56,"Vrms.",115,90,"-",205,240,"-",22,20,20,1,7.4,"-","-",4,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL07AR220M3P51B0",48,56,"Vrms.",115,90,"-",205,240,"-",22,20,20,1,7.4,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59970C0130A070",48,80,"Vrms.",150,117,93,240,288,"-",20,20,20,1,9,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,125,-40,125,"-"]
["Thinking","PPL05200*A363",48,63,"Vrms.",150,"-","-",240,"-","-",20,"-","-",1,"4.5to7","-","-","2.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL05H131E*E",48,60,"Vrms.",130,104,80.599999999999994,195,230.1,249.6,25,20,20,1.2,5,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL07AR8R2M3P51A0",49,56,"Vrms.",165,90,"-",300,240,"-",8.1999999999999993,20,20,1,7.4,"-","-",4,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL07AR8R2M3P51B0",49,56,"Vrms.",165,90,"-",300,240,"-",8.1999999999999993,20,20,1,7.4,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59970C0130A070",49,80,"Vrms.",150,117,93,240,288,"-",20,20,20,1,9,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,125,-40,125,"-"]
["Thinking","PPL05100*A263",49,63,"Vrms.",170,"-","-",340,"-","-",10,"-","-",3,"4.0to6.5","-","-","2.0to4.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL07H171F*E",49,145,"Vrms.",170,136,105.4,255,300.89999999999998,326.40000000000003,19,20,20,1,7,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL07AR8R2M3N54B0",50,56,"Vrms.","-",130,"-","-",350,"-",8.1999999999999993,20,20,1,7.4,"-","-",4,"-","-",5,1.5,1.5,0.5,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59850C0130A070",50,265,"Vrms.",200,160,134,320,384,"-",13,20,20,1.5,13.5,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Thinking","PPL05100*A263",50,63,"Vrms.",170,"-","-",340,"-","-",10,"-","-",3,"4.0to6.5","-","-","2.0to4.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL07H171F*E",50,145,"Vrms.",170,136,105.4,255,300.89999999999998,326.40000000000003,19,20,20,1,7,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL09AR150M3B51A0",51,56,"Vrms.",190,150,"-",340,400,"-",15,20,20,1.2,9.5,"-","-",4,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL09AR150M3B51B0",51,56,"Vrms.",190,150,"-",340,400,"-",15,20,20,1.2,9.5,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL09AR150M3B54B0",51,56,"Vrms.",190,150,"-",340,400,"-",15,20,20,1.2,9.5,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59850C0130A070",51,265,"Vrms.",200,160,134,320,384,"-",13,20,20,1.5,13.5,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Thinking","PPL10130*A3B2",51,220,"Vrms.",200,"-","-",320,"-","-",13,"-","-",1.5,"9.5to12","-","-","3.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL07H211F*E",51,145,"Vrms.",210,168,130.19999999999999,315,371.7,403.2,12,20,20,1.4,7,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL10AR3R9M3N64B0",52,56,"Vrms.","-",210,"-","-",550,"-",3.9,20,20,2,10.5,"-","-",4,"-","-",6.5,1.5,1.5,0.5,0.05,0.05,-10,60,"-","-","Special specification type"]
["Murata","PTGL10AR3R9M3P51A0",52,56,"Vrms.",260,210,"-",470,550,"-",3.9,20,20,2,10.5,"-","-",4,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL10AR3R9M3P51B0",52,56,"Vrms.",260,210,"-",470,550,"-",3.9,20,20,2,10.5,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59960C0130A070",52,80,"Vrms.",250,195,155,380,456,"-",8,20,20,3,11,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,125,-40,125,"-"]
["Thinking","PPL088R0*A363",52,63,"Vrms.",250,"-","-",380,"-","-",8,"-","-",3,"7.5to10","-","-","2.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL09H271F*E",52,145,"Vrms.",270,216,167.4,405,477.9,518.4,8,20,20,2.2000000000000002,8.5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL09AR4R7M3B51A0",53,56,"Vrms.",350,270,"-",600,700,"-",4.7,20,20,2,9.5,"-","-",4,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL09AR4R7M3B51B0",53,56,"Vrms.",350,270,"-",600,700,"-",4.7,20,20,2,9.5,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL09AR4R7M3C64B0",53,56,"Vrms.",350,270,"-",600,700,"-",4.7,20,20,2,9.5,"-","-",4,"-","-",null,null,null,0.65,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59840C0130A070",53,265,"Vrms.",330,264,221.10000000000002,500,600,"-",9,20,20,2.2000000000000002,17.5,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Thinking","PPL129R0*A3B2",53,220,"Vrms.",330,"-","-",500,"-","-",9,"-","-",2.2000000000000002,"11to14","-","-","3.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Murata","PTGL10AR3R9M3B51A0",54,56,"Vrms.",390,300,"-",680,800,"-",3.9,20,20,2,10.5,"-","-",4,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL10AR3R9M3B51B0",54,56,"Vrms.",390,300,"-",680,800,"-",3.9,20,20,2,10.5,"-","-",4,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL10AR3R9M3C61B0",54,56,"Vrms.","-",340,"-","-",800,"-",3.9,20,20,1.5,10.5,"-","-",4,"-","-",6.5,1.5,1.5,0.65,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL10AR3R9M3C64B0",54,56,"Vrms.","-","-","-","-","-","-",3.9,20,20,"-",10.5,"-","-",4,"-","-",6.5,1.5,1.5,0.65,0.05,0.05,-10,60,"-","-","Special specification type"]
["TDK/EPCOS","B59830C0130A070",54,265,"Vrms.",450,360,301.5,680,816,"-",5,20,20,4.0999999999999996,17.5,"-","-",5,"-","-",5,"-","-",0.8,"-","-",0,60,-40,125,"-"]
["Thinking","PPL165R0*A3B2",54,220,"Vrms.",450,"-","-",680,"-","-",5,"-","-",4.0999999999999996,"15to17.5","-","-","3.0to6.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL13H411F*E",54,145,"Vrms.",410,328,254.2,615,725.69999999999993,787.2,4.5999999999999996,20,20,4.5,12.5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL14AR3R3M3B71B0",55,56,"Vrms.",490,380,"-",830,980,"-",3.3,20,20,2.5,14.5,"-","-",4,"-","-",7.5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL14AR3R3M3C01B0",55,56,"Vrms.","-",420,"-","-",990,"-",3.3,20,20,2,14.5,"-","-",4,"-","-",10,1.5,1.5,0.65,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL14AR3R3M3C04B0",55,56,"Vrms.","-",420,"-","-",990,"-",3.3,20,20,2,14.5,"-","-",4,"-","-",10,1.5,1.5,0.65,0.05,0.05,-10,60,"-","-","Special specification type"]
["TDK/EPCOS","B59830C0160A070",55,160,"Vrms.",525,420,351.75,1050,1207.5,"-",3.7,25,25,7,22,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Thinking","PPL123R3*A363",55,63,"Vrms.",450,"-","-",690,"-","-",3.3,"-","-",5.5,"11.5to14","-","-","2.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL17H601FBE",55,145,"Vrms.",600,480,372,900,1062,1152,2.9,20,20,7.2,16.5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"Bulk"]
["Murata","PTGL04AS220K4B51A0",56,60,"Vrms.",145,115,87,193,226,"-",22,10,10,1,4.5,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL4SAS220K4B51A0",56,60,"Vrms.",145,"-",87,193,"-","-",22,10,10,1,4.5,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,125,-40,125,"-"]
["Murata","PTGL04AS220K4B51B0",56,60,"Vrms.",145,115,87,193,226,"-",22,10,10,1,4.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL4SAS220K4B51B0",56,60,"Vrms.",145,"-",87,193,"-","-",22,10,10,1,4.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,125,-40,125,"-"]
["Vishay","PTCCL05H131E*E",56,60,"Vrms.",130,104,80.599999999999994,195,230.1,249.6,25,20,20,1.2,5,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL04AS220K4N51A0",57,60,"Vrms.",112,88,67,149,175,"-",22,10,10,1,4.5,"-","-",3.5,"-","-",5,0.3,0.8,0.5,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL4SAS220K4N51A0",57,60,"Vrms.",112,"-",67,149,"-","-",22,10,10,1,4.5,"-","-",3.5,"-","-",5,0.3,0.8,0.5,0.05,0.05,-30,125,-40,125,"-"]
["Murata","PTGL04AS220K4N51B0",57,60,"Vrms.",112,88,67,149,175,"-",22,10,10,1,4.5,"-","-",3.5,"-","-",5,1.5,1.5,0.5,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL4SAS220K4N51B0",57,60,"Vrms.",112,"-",67,149,"-","-",22,10,10,1,4.5,"-","-",3.5,"-","-",5,1.5,1.5,0.5,0.05,0.05,-30,125,-40,125,"-"]
["Murata","PTGL04AS220K4N52AL",57,null,null,112,"-",67,149,"-","-",22,10,10,1,4.5,"-","-",3.5,"-","-",5,1.5,1.5,0.5,0.05,0.05,-30,125,-40,125,"Special specification type"]
["TDK/EPCOS","B59870C0130A070",57,265,"Vrms.",100,80,67,150,180,"-",50,20,20,0.4,9,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Thinking","PPL05500*A3B2",57,220,"Vrms.",100,"-","-",150,"-","-",50,"-","-",0.4,"4.5to7","-","-","3.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL05H131E*E",57,60,"Vrms.",130,104,80.599999999999994,195,230.1,249.6,25,20,20,1.2,5,"-","-",4,"-","-",5,"-","-",0.6,0.05,0.05,-40,85,-40,150,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL05AS100K4B51A0",58,60,"Vrms.",215,170,"-",286,335,"-",10,10,10,1.5,5.5,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL5SAS100K4B51A0",58,60,"Vrms.",215,"-",129,286,335,"-",10,10,10,1.5,5.5,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL05AS100K4B51B0",58,60,"Vrms.",215,170,"-",286,335,"-",10,10,10,1.5,5.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL5SAS100K4B51B0",58,60,"Vrms.",215,"-",129,286,335,"-",10,10,10,1.5,5.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Vishay","PTCCL07H211F*E",58,145,"Vrms.",210,168,130.19999999999999,315,371.7,403.2,12,20,20,1.4,7,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL07AS5R6K4N51A0",59,60,"Vrms.",236,186,142,314,368,"-",5.6,10,10,2.2000000000000002,7.3,"-","-",3.5,"-","-",5,0.3,0.8,0.5,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL7SAS5R6K4N51A0",59,60,"Vrms.",236,"-",142,314,"-","-",5.6,10,10,2.2000000000000002,7.3,"-","-",3.5,"-","-",5,0.3,0.8,0.5,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL07AS5R6K4N51B0",59,60,"Vrms.",236,186,142,314,368,"-",5.6,10,10,2.2000000000000002,7.3,"-","-",3.5,"-","-",5,1.5,1.5,0.5,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL7SAS5R6K4N51B0",59,60,"Vrms.",236,"-",142,314,"-","-",5.6,10,10,2.2000000000000002,7.3,"-","-",3.5,"-","-",5,1.5,1.5,0.5,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL07AS5R6K4N52AL",59,60,"Vrms.","-","-","-","-","-","-",5.6,10,10,2.2000000000000002,7.3,"-","-",3.5,"-","-",5,0.3,0.8,0.5,0.05,0.05,-30,85,-40,125,"Special specification type"]
["Vishay","PTCCL07H211F*E",59,145,"Vrms.",210,168,130.19999999999999,315,371.7,403.2,12,20,20,1.4,7,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL07AS5R6K4B51A0",60,60,"Vrms.",290,229,174,386,452,"-",5.6,10,10,3,7.3,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL7SAS5R6K4B51A0",60,60,"Vrms.",290,"-",174,386,"-","-",5.6,10,10,3,7.3,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL07AS5R6K4B51B0",60,60,"Vrms.",290,229,174,386,452,"-",5.6,10,10,3,7.3,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL7SAS5R6K4B51B0",60,60,"Vrms.",290,"-",174,386,"-","-",5.6,10,10,3,7.3,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-40,125,-40,125,"-"]
["TDK/EPCOS","B59960C0130A070",60,80,"Vrms.",250,195,155,380,456,"-",8,20,20,3,11,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,125,-40,125,"-"]
["Thinking","PPL088R0*A363",60,63,"Vrms.",250,"-","-",380,"-","-",8,"-","-",3,"7.5to10","-","-","2.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL09H271F*E",60,145,"Vrms.",270,216,167.4,405,477.9,518.4,8,20,20,2.2000000000000002,8.5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL09AS5R0K4B74B1",61,60,"Vrms.",341,279,"-",472,539,"-",5,10,10,3.3,9.3000000000000007,"-","-",4.5,"-","-",7.5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"Special specification type"]
["Vishay","PTCCL13H411F*E",61,145,"Vrms.",410,328,254.2,615,725.69999999999993,787.2,4.5999999999999996,20,20,4.5,12.5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL09AS3R3K4B51A0",62,60,"Vrms.",421,333,253,560,656,"-",3.3,10,10,4,9.3000000000000007,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL9SAS3R3K4B51A0",62,60,"Vrms.",421,"-",253,560,656,"-",3.3,10,10,4,9.3000000000000007,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL09AS3R3K4B51B0",62,60,"Vrms.",421,333,253,560,656,"-",3.3,10,10,4,9.3000000000000007,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL9SAS3R3K4B51B0",62,60,"Vrms.",421,"-",253,560,656,"-",3.3,10,10,4,9.3000000000000007,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL09AS3R3K4B74B1",62,60,"Vrms.",421,333,"-",560,656,"-",3.3,10,10,4,9.3000000000000007,"-","-",4.5,"-","-",7.5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"Special specification type"]
["Vishay","PTCCL13H411F*E",62,145,"Vrms.",410,328,254.2,615,725.69999999999993,787.2,4.5999999999999996,20,20,4.5,12.5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL12AS2R2K4B51A0",63,60,"Vrms.",556,439,"-",739,867,"-",2.2000000000000002,10,10,5,11.5,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGLCSAS2R2K4B51A0",63,60,"Vrms.",556,"-",334,739,"-","-",2.2000000000000002,10,10,5,11.5,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL12AS2R2K4B51B0",63,60,"Vrms.",556,439,"-",739,867,"-",2.2000000000000002,10,10,5,11.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGLCSAS2R2K4B51B0",63,60,"Vrms.",556,"-",334,739,"-","-",2.2000000000000002,10,10,5,11.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL12AS2R2K4B52AL",63,60,"Vrms.",556,439,"-",739,867,"-",2.2000000000000002,10,10,5,11.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"Special specification type"]
["Thinking","PPL123R3*A363",63,63,"Vrms.",450,"-","-",690,"-","-",3.3,"-","-",5.5,"11.5to14","-","-","2.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL13H451F*E",63,145,"Vrms.",450,360,279,675,796.5,864,3.8,20,20,5,12.5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL05AR550H4P51A0",64,80,"Vrms.",62,50,"-",115,135,"-",55,25,25,0.7,5.5,"-","-",4.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL05AR550H4P51B0",64,80,"Vrms.",62,50,"-",115,135,"-",55,25,25,0.7,5.5,"-","-",4.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59990C0120A070",64,80,"Vrms.",50,37.5,27.500000000000004,100,120,"-",55,25,25,0.7,4,"-","-",3.5,"-","-",5,"-","-",0.5,"-","-",-40,125,-40,125,"-"]
["Thinking","PPL05121*A4A1",64,110,"Vrms.",65,"-","-",130,"-","-",120,"-","-",0.3,"4.5to7","-","-","3.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL05H650F*E",64,145,"Vrms.",65,52,40.299999999999997,100,118,128,115,20,20,0.3,5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL07AR250H4B51A0",65,80,"Vrms.",140,110,"-",260,300,"-",25,25,25,1,7.4,"-","-",4.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL07AR250H4B51B0",65,80,"Vrms.",140,110,"-",260,300,"-",25,25,25,1,7.4,"-","-",4.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["Thinking","PPL05280*A4A1",65,110,"Vrms.",130,"-","-",260,"-","-",28,"-","-",0.6,"4.5to7","-","-","3.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL07H171F*E",65,145,"Vrms.",170,136,105.4,255,300.89999999999998,326.40000000000003,19,20,20,1,7,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL09AR9R4H4B51A0",66,80,"Vrms.",240,190,"-",450,530,"-",9.4,25,25,3,9.5,"-","-",4.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL09AR9R4H4B51B0",66,80,"Vrms.",240,190,"-",450,530,"-",9.4,25,25,3,9.5,"-","-",4.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59970C0120A070",66,80,"Vrms.",150,112.5,82.5,300,360,"-",9.4,25,25,3,9,"-","-",3.5,"-","-",5,"-","-",0.6,"-","-",-40,125,-40,125,"-"]
["Thinking","PPL089R4*A4A1",66,110,"Vrms.",250,"-","-",500,"-","-",9.4,"-","-",2,"7.5to10","-","-","3.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL09H271F*E",66,145,"Vrms.",270,216,167.4,405,477.9,518.4,8,20,20,2.2000000000000002,8.5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL05AR181M7N52A0",67,125,"Vrms.","-","-","-","-","-","-",180,20,20,"-","-","-","-","-","-","-",5,0.3,0.8,0.5,0.05,0.05,"-","-","-","-","-"]
["Murata","PTGL05AR181M7P52A0",67,125,"Vrms.",38,30,"-",64,75,"-",180,20,20,0.3,6,"-","-",5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL05AR181M7P52B0",67,125,"Vrms.",38,30,"-",64,75,"-",180,20,20,0.3,6,"-","-",5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59890C0120A070",67,265,"Vrms.",30,22.5,16.5,60,72,"-",150,25,25,0.2,4,"-","-",5,"-","-",5,"-","-",0.5,"-","-",0,60,-40,125,"-"]
["Thinking","PPL06301*A2B2",67,220,"Vrms.",33,"-","-",66,"-","-",300,"-","-",0.2,"5.5to8","-","-","3.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL05H470F*E",67,145,"Vrms.",47,37.6,29.14,70,82.6,89.600000000000009,240,20,20,0.2,5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL09AR220M6B52A0",68,125,"Vrms.",175,135,"-",290,340,"-",22,20,20,0.8,10,"-","-",5.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL09AR220M6B52B0",68,125,"Vrms.",175,135,"-",290,340,"-",22,20,20,0.8,10,"-","-",5.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["Vishay","PTCCL07H171F*E",68,145,"Vrms.",170,136,105.4,255,300.89999999999998,326.40000000000003,19,20,20,1,7,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL14AR100M6B72B0",69,125,"Vrms.",280,220,"-",475,550,"-",10,20,20,1.2,15,"-","-",5.5,"-","-",7.5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59840C0130A070",69,265,"Vrms.",330,264,221.10000000000002,500,600,"-",9,20,20,2.2000000000000002,17.5,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Thinking","PPL09120*A4B2",69,220,"Vrms.",250,"-","-",375,"-","-",12,"-","-",1.5,"8.5to11","-","-","3.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL09H271F*E",69,145,"Vrms.",270,216,167.4,405,477.9,518.4,8,20,20,2.2000000000000002,8.5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL04AS560K6B51A0",70,140,"Vrms.",94,74,"-",125,147,"-",56,10,10,0.5,5.5,"-","-",4.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL4SAS560K6B51A0",70,140,"Vrms.",94,"-",56,125,147,"-",56,10,10,0.5,5.5,"-","-",4.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL04AS560K6B51B0",70,140,"Vrms.",94,74,"-",125,147,"-",56,10,10,0.5,5.5,"-","-",4.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL4SAS560K6B51B0",70,140,"Vrms.",94,"-",56,125,147,"-",56,10,10,0.5,5.5,"-","-",4.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL04AS560K6B52AL",70,140,"Vrms.",94,"-",56,125,147,"-",56,10,10,0.5,5.5,"-","-",4.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-40,125,-40,125,"Special specification type"]
["TDK/EPCOS","B59873C0120A570",70,265,"Vrms.",90,67.5,49.500000000000007,140,168,"-",27,20,20,1,9,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Vishay","PTCCL05H930F*E",70,145,"Vrms.",93,74.400000000000006,57.66,140,165.2,179.20000000000002,55,20,20,0.45,5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL07AR330M6A51B0",71,140,"Vrms.",130,100,"-",200,230,"-",33,20,20,0.5,7.4,"-","-",6,"-","-",5,1.5,1.5,0.5,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL07AR330M6A54B3",71,140,"VDC",130,100,"-",200,230,"-",33,20,20,0.5,7.4,"-","-",6,"-","-",5,1.5,1.5,0.5,0.05,0.05,-10,60,"-","-","Special specification type"]
["Murata","PTGL07AR330M6B51A0",71,140,"Vrms.",130,100,"-",200,230,"-",33,20,20,0.5,7.4,"-","-",6,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Thinking","PPL08250*A3B2",71,220,"Vrms.",140,"-","-",230,"-","-",25,"-","-",1,"7.5to10","-","-","3.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL05H131F*E",71,145,"Vrms.",130,104,80.599999999999994,195,230.1,249.6,28,20,20,0.6,5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL05AS270K6B51A0",72,140,"Vrms.",134,106,80,178,209,"-",27,10,10,1,5.5,"-","-",4.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL5SAS270K6B51A0",72,140,"Vrms.",134,"-",80,178,209,"-",27,10,10,1,5.5,"-","-",4.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL05AS270K6B51B0",72,140,"Vrms.",134,106,80,178,209,"-",27,10,10,1,5.5,"-","-",4.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL5SAS270K6B51B0",72,140,"Vrms.",134,"-",80,178,209,"-",27,10,10,1,5.5,"-","-",4.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Vishay","PTCCL05H131F*E",72,145,"Vrms.",130,104,80.599999999999994,195,230.1,249.6,28,20,20,0.6,5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL07AS150K6B51A0",73,140,"Vrms.",187,148,112,249,292,"-",15,10,10,1.5,7.3,"-","-",4.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL7SAS150K6B51A0",73,140,"Vrms.",187,"-",112,249,"-","-",15,10,10,1.5,7.3,"-","-",4.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL07AS150K6B51B0",73,140,"Vrms.",187,148,112,249,292,"-",15,10,10,1.5,7.3,"-","-",4.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL7SAS150K6B51B0",73,140,"Vrms.",187,"-",112,249,"-","-",15,10,10,1.5,7.3,"-","-",4.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL07AS150K6B52AL",73,140,"Vrms.",187,148,112,249,292,"-",15,10,10,1.5,7.3,"-","-",4.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-40,125,"Special specification type"]
["Murata","PTGL07AS150K6B54B0",73,140,"Vrms.",187,148,"-",249,292,"-",15,10,10,1.5,7.3,"-","-",4.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Vishay","PTCCL07H171F*E",73,145,"Vrms.",170,136,105.4,255,300.89999999999998,326.40000000000003,19,20,20,1,7,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL09AR220M6C61B0",74,140,"Vrms.",180,140,"-",280,330,"-",22,20,20,1,9.6,"-","-",6,"-","-",6.5,1.5,1.5,0.65,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59850C0130A070",74,265,"Vrms.",200,160,134,320,384,"-",13,20,20,1.5,13.5,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Thinking","PPL10130*A3B2",74,220,"Vrms.",200,"-","-",320,"-","-",13,"-","-",1.5,"9.5to12","-","-","3.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL07H171F*E",74,145,"Vrms.",170,136,105.4,255,300.89999999999998,326.40000000000003,19,20,20,1,7,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL10AR150M6C61B0",75,140,"Vrms.",220,170,"-",345,400,"-",15,20,20,1,11.6,"-","-",6,"-","-",6.5,1.5,1.5,0.65,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL10AR150M6C64B0",75,140,"Vrms.",220,170,"-",345,400,"-",15,20,20,1,11.6,"-","-",6,"-","-",6.5,1.5,1.5,0.65,0.05,0.05,-10,60,"-","-","Special specification type"]
["TDK/EPCOS","B59850C0130A070",75,265,"Vrms.",200,160,134,320,384,"-",13,20,20,1.5,13.5,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Thinking","PPL10130*A3B2",75,220,"Vrms.",200,"-","-",320,"-","-",13,"-","-",1.5,"9.5to12","-","-","3.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL09H251F*E",75,145,"Vrms.",250,200,155,375,442.5,480,9.4,20,20,2,8.5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL09AS120K6B51A0",76,140,"Vrms.",244,192,"-",324,380,"-",12,10,10,2,9.3000000000000007,"-","-",4.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL9SAS120K6B51A0",76,140,"Vrms.",244,"-",146,324,"-","-",12,10,10,2,9.3000000000000007,"-","-",4.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL09AS120K6B51B0",76,140,"Vrms.",244,192,"-",324,380,"-",12,10,10,2,9.3000000000000007,"-","-",4.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL9SAS120K6B51B0",76,140,"Vrms.",244,"-",146,324,"-","-",12,10,10,2,9.3000000000000007,"-","-",4.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL09AS120K6B74B1",76,140,"Vrms.",244,192,"-",324,380,"-",12,10,10,2,9.3000000000000007,"-","-",4.5,"-","-",7.5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"Special specification type"]
["Thinking","PPL09120*A4B2",76,220,"Vrms.",250,"-","-",375,"-","-",12,"-","-",1.5,"8.5to11","-","-","3.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL09H251F*E",76,145,"Vrms.",250,200,155,375,442.5,480,9.4,20,20,2,8.5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL12AS9R0K6B04B2",77,140,"Vrms.",262,215,"-",360,411,"-",9,10,10,3,12.5,"-","-",4.5,"-","-",10,1.5,1.5,0.6,0.05,0.05,-20,85,"-","-","Special specification type"]
["Murata","PTGL12AS100Q6B74B2",77,140,"Vrms.",267,220,"-",340,453,"-",10,5.5,15.5,3,12,"-","-",4.5,"-","-",7.5,1.5,1.5,0.6,0.05,0.05,-20,85,-30,85,"-"]
["Vishay","PTCCL09H271F*E",77,145,"Vrms.",270,216,167.4,405,477.9,518.4,8,20,20,2.2000000000000002,8.5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL09AS7R6K6B51A0",78,140,"Vrms.",287,227,"-",382,447,"-",7.6,10,10,2.2000000000000002,9.3000000000000007,"-","-",4.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL9SAS7R6K6B51A0",78,140,"Vrms.",287,"-",172,382,"-","-",7.6,10,10,2.2000000000000002,9.3000000000000007,"-","-",4.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL09AS7R6K6B51B0",78,140,"Vrms.",287,227,"-",382,447,"-",7.6,10,10,2.2000000000000002,9.3000000000000007,"-","-",4.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL9SAS7R6K6B51B0",78,140,"Vrms.",287,"-",172,382,"-","-",7.6,10,10,2.2000000000000002,9.3000000000000007,"-","-",4.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL09AS7R6K6B74B1",78,140,"Vrms.",287,227,"-",382,447,"-",7.6,10,10,2.2000000000000002,9.3000000000000007,"-","-",4.5,"-","-",7.5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"Special specification type"]
["Thinking","PPL09120*A4B2",78,220,"Vrms.",250,"-","-",375,"-","-",12,"-","-",1.5,"8.5to11","-","-","3.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL09H271F*E",78,145,"Vrms.",270,216,167.4,405,477.9,518.4,8,20,20,2.2000000000000002,8.5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL12AR100M6C01B0",79,140,"Vrms.",290,220,"-",440,510,"-",10,20,20,1,13,"-","-",6,"-","-",10,1.5,1.5,0.65,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL12AR100M6C52B0",79,140,"Vrms.",290,220,"-",440,510,"-",10,20,20,1,13,"-","-",6,"-","-",5,1.5,1.5,0.65,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59840C0130A070",79,265,"Vrms.",330,264,221.10000000000002,500,600,"-",9,20,20,2.2000000000000002,17.5,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Thinking","PPL09120*A4B2",79,220,"Vrms.",250,"-","-",375,"-","-",12,"-","-",1.5,"8.5to11","-","-","3.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL09H271F*E",79,145,"Vrms.",270,216,167.4,405,477.9,518.4,8,20,20,2.2000000000000002,8.5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL12AS8R0K6B74B2",80,140,"Vrms.",292,237,"-",414,480,"-",8,10,10,3,12,"-","-",4.5,"-","-",7.5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL12AS6R0K6B04B2",80,140,"Vrms.",300,250,"-",465,530,"-",6,10,10,3,12,"-","-",4.5,"-","-",10,1.5,1.5,0.6,0.05,0.05,-20,85,"-","-","-"]
["Murata","PTGL12AS6R0K6B74B2",80,140,"Vrms.",300,250,"-",465,530,"-",6,10,10,3,12,"-","-",4.5,"-","-",7.5,1.5,1.5,0.6,0.05,0.05,-20,85,"-","-","-"]
["Murata","PTGL12AS6R3K6B74B2",80,140,"Vrms.",310,250,"-",445,520,"-",6,10,10,3,12,"-","-",4.5,"-","-",7.5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"Special specification type"]
["Thinking","PPL129R0*A3B2",80,220,"Vrms.",330,"-","-",500,"-","-",9,"-","-",2.2000000000000002,"11to14","-","-","3.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL11H321F*E",80,145,"Vrms.",320,256,198.4,480,566.4,614.4,6.7,20,20,3,10.5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL13AR6R8M6C01B0",81,140,"Vrms.",370,290,"-",575,670,"-",6.8,20,20,1,14,"-","-",6,"-","-",10,1.5,1.5,0.65,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL12AS4R7K6B51A0",81,140,"Vrms.",393,310,"-",523,613,"-",4.7,10,10,3.5,11.5,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGLCSAS4R7K6B51A0",81,140,"Vrms.",393,"-",236,523,"-","-",4.7,10,10,3.5,11.5,"-","-",3.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL12AS4R7K6B51B0",81,140,"Vrms.",393,310,"-",523,613,"-",4.7,10,10,3.5,11.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGLCSAS4R7K6B51B0",81,140,"Vrms.",393,"-",236,523,"-","-",4.7,10,10,3.5,11.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-40,125,-40,125,"-"]
["Murata","PTGL12AS4R7K6B74B2",81,140,"Vrms.",393,310,"-",523,613,"-",4.7,10,10,3.5,11.5,"-","-",3.5,"-","-",7.5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"Special specification type"]
["Murata","PTGL12AS4R7K6B52A0",81,140,"Vrms.",393,310,"-",523,613,"-",4.7,10,10,3.5,11.5,"-","-",3.5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"-"]
["TDK/EPCOS","B59840C0130A070",81,265,"Vrms.",330,264,221.10000000000002,500,600,"-",9,20,20,2.2000000000000002,17.5,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Thinking","PPL129R0*A3B2",81,220,"Vrms.",330,"-","-",500,"-","-",9,"-","-",2.2000000000000002,"11to14","-","-","3.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL11H361F*E",81,145,"Vrms.",360,288,223.2,540,637.19999999999993,691.2,5.3,20,20,3.5,10.5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL16AR5R6M6C01B0",89,140,"Vrms.",440,340,"-",670,780,"-",5.6,20,20,2,17,"-","-",6,"-","-",10,1.5,1.5,0.65,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL16AR5R6M6C01B3",89,140,"Vrms.",440,340,"-",670,780,"-",5.6,20,20,2,17,"-","-",6,"-","-",10,1.5,1.5,0.65,0.05,0.05,-10,60,"-","-","Special specification type"]
["Murata","PTGL16AR5R6M6C04B2",89,140,"Vrms.",440,340,"-",670,780,"-",5.6,20,20,2,17,"-","-",6,"-","-",10,1.5,1.5,0.65,0.05,0.05,-10,60,"-","-","Special specification type"]
["TDK/EPCOS","B59830C0130A070",89,265,"Vrms.",450,360,301.5,680,816,"-",5,20,20,4.0999999999999996,17.5,"-","-",5,"-","-",5,"-","-",0.8,"-","-",0,60,-40,125,"-"]
["Thinking","PPL165R0*A3B2",89,220,"Vrms.",450,"-","-",680,"-","-",5,"-","-",4.0999999999999996,"15to17.5","-","-","3.0to6.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL13H451F*E",89,145,"Vrms.",450,360,279,675,796.5,864,3.8,20,20,5,12.5,"-","-",5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL05AR301M7N52B0",89,160,"Vrms.","-",22,"-","-",55,"-",300,20,20,0.3,6,"-","-",4.5,"-","-",5,1.5,1.5,0.5,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL05AR331M7A52B0",89,160,"Vrms.","-",22,"-","-",55,"-",300,20,20,0.3,6,"-","-",4.5,"-","-","-","-","-","-","-","-","-","-","-","-","-"]
["TDK/EPCOS","B59883C0120A070",89,265,"Vrms.",35,26.25,19.25,70,84,"-",120,25,25,0.4,4,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Thinking","PPL05251*A2D0",89,400,"Vrms.",32,"-","-",65,"-","-",250,"-","-",0.3,"4.5to7","-","-","3.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL05H390H*E",89,265,"Vrms.",39,31.200000000000003,24.18,59,69.61999999999999,75.52,260,20,20,0.3,5,"-","-",5.5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL06BB220N8B52A0",90,250,"Vrms.","-","100(50℃)","-",260,"-","-",22,30,30,0.5,7.5,"-","-",6,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL06BB220N8B52B0",90,250,"Vrms.","-","100(50℃)","-",260,"-","-",22,30,30,0.5,7.5,"-","-",6,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59860C0120A070",90,265,"Vrms.",140,105,77,280,336,"-",15,25,25,1.5,11,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Thinking","PPL07220NA0B5",90,250,"Vrms.",100,"-","-",260,"-","-",22,"-","-",0.5,"6.5to9","-","-","3.0to6.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL07H141H*E",90,265,"Vrms.",140,112,86.8,210,247.79999999999998,268.8,29,20,20,0.8,7,"-","-",5.5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL07BB220N0B52A0",91,250,"Vrms.",130,90,"-",250,300,"-",22,30,30,0.5,8,"-","-",6,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL07BB220N0B52B0",91,250,"Vrms.",130,90,"-",250,300,"-",22,30,30,0.5,8,"-","-",6,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59860C0120A070",91,265,"Vrms.",140,105,77,280,336,"-",15,25,25,1.5,11,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Thinking","PPL07220NA0B5",91,250,"Vrms.",100,"-","-",260,"-","-",22,"-","-",0.5,"6.5to9","-","-","3.0to6.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL07H141H*E",91,265,"Vrms.",140,112,86.8,210,247.79999999999998,268.8,29,20,20,0.8,7,"-","-",5.5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL10BB120N0P52A0",92,250,"Vrms.",130,90,"-",260,300,"-",12,30,30,0.6,11,"-","-",6,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","Special specification type"]
["TDK/EPCOS","B59860C0130A070",92,265,"Vrms.",140,112,93.800000000000011,230,276,"-",25,20,20,1,11,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Thinking","PPL08250*A3B2",92,220,"Vrms.",140,"-","-",230,"-","-",25,"-","-",1,"7.5to10","-","-","3.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL07H141H*E",92,265,"Vrms.",140,112,86.8,210,247.79999999999998,268.8,29,20,20,0.8,7,"-","-",5.5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL05AR121M9N51A0",93,265,"Vrms.",47,35,"-",75,85,"-",120,20,20,0.3,6.5,"-","-",6.5,"-","-",5,0.3,0.8,0.5,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL05AR121M9N51B0",93,265,"Vrms.",47,35,"-",75,85,"-",120,20,20,0.3,6.5,"-","-",6.5,"-","-",5,1.5,1.5,0.5,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL05AR121M9N51B1",93,265,"Vrms.",47,35,"-",75,85,"-",120,20,20,0.3,6.5,"-","-",6.5,"-","-",5,1.5,1.5,0.5,0.05,0.05,-10,60,-40,125,"Special specification type"]
["TDK/EPCOS","B59772C0120A070",93,260,"Vrms.",43,32.25,23.650000000000002,86,103.2,"-",150,25,25,2.8,9,"-","-",7.5,"-","-",5,"-","-",0.6,"-","-",-20,85,-40,125,"-"]
["Thinking","PPL08151*A2C8",93,380,"Vrms.",43,"-","-",86,"-","-",150,"-","-",1.4,"7.5to10","-","-","4.5to7.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL05H390H*E",93,265,"Vrms.",39,31.200000000000003,24.18,59,69.61999999999999,75.52,260,20,20,0.3,5,"-","-",5.5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL05AR151H8P52A0",94,265,"Vrms.",35,28,"-",65,78,"-",150,25,25,0.2,6,"-","-",6,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL05AR151H8P52B0",94,265,"Vrms.",35,28,"-",65,78,"-",150,25,25,0.2,6,"-","-",6,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59880C0130A070",94,265,"Vrms.",55,44,36.85,90,108,"-",160,20,20,0.2,6.5,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Thinking","PPL05251*A2D0",94,400,"Vrms.",32,"-","-",65,"-","-",250,"-","-",0.3,"4.5to7","-","-","3.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL05H390H*E",94,265,"Vrms.",39,31.200000000000003,24.18,59,69.61999999999999,75.52,260,20,20,0.3,5,"-","-",5.5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL05AR181M9N52A0",95,265,"Vrms.",37,29,"-",60,70,"-",180,20,20,0.3,6.5,"-","-",6.5,"-","-",5,0.3,0.8,0.5,0.05,0.05,-10,60,-30,85,"-"]
["Murata","PTGL05AR181M9N51B0",95,265,"Vrms.",37,29,"-",60,70,"-",180,20,20,0.3,6.5,"-","-",6.5,"-","-",5,1.5,1.5,0.5,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL05AR181M9N51B1",95,265,"Vrms.",37,29,"-",60,70,"-",180,20,20,0.3,6.5,"-","-",6.5,"-","-",5,1.5,1.5,0.5,0.05,0.05,-10,60,-40,125,"Special specification type"]
["Murata","PTGL05AR181M9N51B2",95,265,"Vrms.",37,29,"-",60,70,"-",180,20,20,0.3,6.5,"-","-",6.5,"-","-",5,1.5,1.5,0.5,0.05,0.05,-10,60,-40,125,"Special specification type"]
["Murata","PTGL05AR181M9N52B0",95,265,"Vrms.",37,29,"-",60,70,"-",180,20,20,0.3,6.5,"-","-",6.5,"-","-",5,1.5,1.5,0.5,0.05,0.05,-10,60,-30,85,"-"]
["TDK/EPCOS","B59883C0120A070",95,265,"Vrms.",35,26.25,19.25,70,84,"-",120,25,25,0.4,4,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Thinking","PPL06301*A2B2",95,220,"Vrms.",33,"-","-",66,"-","-",300,"-","-",0.2,"5.5to8","-","-","3.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL05H390H*E",95,265,"Vrms.",39,31.200000000000003,24.18,59,69.61999999999999,75.52,260,20,20,0.3,5,"-","-",5.5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL05BD102N9N51A0",96,265,"Vrms.","-",5,"-","-",24,"-",1000,30,30,0.2,6,"-","-",5,"-","-",5,0.3,0.8,0.5,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL05BD102N9N51B0",96,265,"Vrms.","-",5,"-","-",24,"-",1000,30,30,0.2,6,"-","-",5,"-","-",5,1.5,1.5,0.5,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL05BD102N9N52A0",96,265,"Vrms.","-",5,"-","-",24,"-",1000,30,30,0.2,6,"-","-",5,"-","-",5,0.3,0.8,0.5,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL05BD102N9N52B0",96,265,"Vrms.","-",5,"-","-",24,"-",1000,30,30,0.2,6,"-","-",5,"-","-",5,1.5,1.5,0.5,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59886C0120A070",96,550,"Vrms.",12,9,6.6000000000000005,24,28.799999999999997,"-",1500,25,25,0.1,6.5,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Vishay","PTCCL05H150H*E",96,265,"Vrms.",15,12,9.3000000000000007,23,27.139999999999997,29.44,1900,20,20,0.11,5,"-","-",5.5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL07AS201M0N51A0",97,265,"Vrms.",43,35,"-",76,"90(-20ﾟC)","-",200,20,20,1.6,7.3,"-","-",6,"-","-",5,0.3,0.8,0.5,0.05,0.05,-20,85,-40,85,"-"]
["Murata","PTGL07AS201M0N51B0",97,265,"Vrms.",43,35,"-",76,"90(-20ﾟC)","-",200,20,20,7.3,7.3,"-",null,6,"-","-",5,1.5,1.5,0.5,0.05,0.05,-20,85,-40,85,"-"]
["TDK/EPCOS","B59772C0120A070",97,260,"Vrms.",43,32.25,23.650000000000002,86,103.2,"-",150,25,25,2.8,9,"-","-",7.5,"-","-",5,"-","-",0.6,"-","-",-20,85,-40,125,"-"]
["Thinking","PPL11800*A2C8 ",97,380,"Vrms.",69,"-","-",137,"-","-",80,"-","-",2,"10.5to13","-","-","4.5to7.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Murata","PTGL07AR650H8B52A0",98,265,"Vrms.",84,68,"-",162,190,"-",65,25,25,0.1,8,"-","-",6,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL07AR650H8B52B0",98,265,"Vrms.",84,68,"-",162,190,"-",65,25,25,0.1,8,"-","-",6,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59875C0120A570",98,265,"Vrms.",80,60,44,120,144,"-",39,20,20,1,9,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Thinking","PPL11500*A2C8",98,380,"Vrms.",87,"-","-",173,"-","-",50,"-","-",2,"10.5to13","-","-","4.5to7.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL05H950H*E",98,265,"Vrms.",95,76,58.9,143,168.73999999999998,183.04,56,20,20,0.6,5,"-","-",5.5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL07AR820M9A51B0",99,265,"Vrms.",75,60,"-",125,150,"-",82,20,20,0.5,8.1999999999999993,"-","-",6.5,"-","-",5,1.5,1.5,0.5,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL07AR820M9B51A0",99,265,"Vrms.","-",60,"-",125,150,"-",82,20,20,0.5,8.1999999999999993,"-","-",6.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL07AR820M9B52A0",99,265,"Vrms.","-",60,"-","-",150,"-",82,20,20,0.5,8.1999999999999993,"-","-",6.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","Special specification type"]
["TDK/EPCOS","B59875C0120A570",99,265,"Vrms.",80,60,44,120,144,"-",39,20,20,1,9,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Vishay","PTCCL05H760H*E",99,265,"Vrms.",76,60.800000000000004,47.12,115,135.69999999999999,147.20000000000002,85,20,20,0.55000000000000004,5,"-","-",5.5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL07AR700H8B52A0",100,265,"Vrms.",85,66,"-",160,185,"-",70,25,25,0.4,8,"-","-",6,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL07AR700H8B52B0",100,265,"Vrms.",85,66,"-",160,185,"-",70,25,25,0.4,8,"-","-",6,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL07AR700H8B52B1",100,265,"Vrms.","-",66,"-","-",185,"-",70,25,25,0.4,8,"-","-",6,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","Special specification type"]
["TDK/EPCOS","B59875C0120A570",100,265,"Vrms.",80,60,44,120,144,"-",39,20,20,1,9,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Thinking","PPL11500*A2C8",100,380,"Vrms.",87,"-","-",173,"-","-",50,"-","-",2,"10.5to13","-","-","4.5to7.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL05H950H*E",100,265,"Vrms.",95,76,58.9,143,168.73999999999998,183.04,56,20,20,0.6,5,"-","-",5.5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL07AR560M9A51B0",101,265,"Vrms.",95,80,"-",165,190,"-",56,20,20,0.8,8.1999999999999993,"-","-",6.5,"-","-",5,1.5,1.5,0.5,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL07AR560M9A52B0",101,265,"Vrms.",95,80,"-",165,190,"-",36,20,20,0.8,8.1999999999999993,"-","-",6.5,"-","-",5,1.5,1.5,0.5,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL07AR560M9A54B0",101,265,"Vrms.",95,80,"-",165,190,"-",56,20,20,0.8,8.1999999999999993,"-","-",6.5,"-","-",5,1.5,1.5,0.5,0.05,0.05,-10,60,"-","-","Special specification type"]
["Murata","PTGL07AR560M9B51A0",101,265,"Vrms.","-",80,"-","-",190,"-",56,20,20,0.8,8.1999999999999993,"-","-",6.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59870C0130A070",101,265,"Vrms.",100,80,67,150,180,"-",50,20,20,0.4,9,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Thinking","PPL05500*A3B2",101,220,"Vrms.",100,"-","-",150,"-","-",50,"-","-",0.4,"4.5to7","-","-","3.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL05H950H*E",101,265,"Vrms.",95,76,58.9,143,168.73999999999998,183.04,56,20,20,0.6,5,"-","-",5.5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL07AR450H8B52A0",102,265,"Vrms.",105,80,"-",200,220,"-",45,25,25,1,8,"-","-",6,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL07AR450H8B52B0",102,265,"Vrms.",105,80,"-",200,220,"-",45,25,25,1,8,"-","-",6,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59870C0130A070",102,265,"Vrms.",100,80,67,150,180,"-",50,20,20,0.4,9,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Thinking","PPL10390*A2B7",102,270,"Vrms.",100,"-","-",250,"-","-",39,"-","-",1.2,"9.5to12","-","-","3.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL07H111H*E",102,265,"Vrms.",110,88,68.2,165,194.7,211.20000000000002,48,20,20,0.65,7,"-","-",5.5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL09AR390N0B51A0",103,265,"Vrms.",115,100,"-",245,280,"-",39,30,30,1.2,10,"-","-",6,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL09AR390N0B52A0",103,265,"Vrms.",115,100,"-",245,280,"-",39,30,30,0.6,10,"-","-",6,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Thinking","PPL10390*A2B7",103,270,"Vrms.",100,"-","-",250,"-","-",39,"-","-",1.2,"9.5to12","-","-","3.0to5.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL07H141H*E",103,265,"Vrms.",140,112,86.8,210,247.79999999999998,268.8,29,20,20,0.8,7,"-","-",5.5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL09AR390M9C61B0",104,265,"Vrms.",130,100,"-",210,240,"-",39,20,20,1.2,10,"-","-",6.5,"-","-",6.5,1.5,1.5,0.65,0.05,0.05,-10,60,"-","-","-"]
["Thinking","PPL11250*A2C8",104,380,"Vrms.",123,"-","-",245,"-","-",25,"-","-",2,"10.5to13","-","-","4.5to7.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL07H141H*E",104,265,"Vrms.",140,112,86.8,210,247.79999999999998,268.8,29,20,20,0.8,7,"-","-",5.5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL09AR250H8B52A0",105,265,"Vrms.",150,118,"-",290,330,"-",25,25,25,1,10,"-","-",6,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL09AR250H8B52B0",105,265,"Vrms.",150,118,"-",290,330,"-",25,25,25,1,10,"-","-",6,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL09AR250H8B52B1",105,265,"Vrms.",150,118,"-",290,330,"-",25,25,25,1,10,"-","-",6,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","Special specification type"]
["Murata","PTGL09AR250H8B62B0",105,265,"Vrms.",150,118,"-",290,330,"-",25,25,25,1,10,"-","-",6,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["TDK/EPCOS","B59860C0120A570",105,265,"Vrms.",170,127.5,93.500000000000014,260,312,"-",15,20,20,1.5,11,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Thinking","PPL16500*A2B7",105,270,"Vrms.",160,"-","-",320,"-","-",50,"-","-",4,"14to18","-","-","3.0to7.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL09H171H*E",105,265,"Vrms.",170,136,105.4,255,300.89999999999998,326.40000000000003,22,20,20,0.9,8.5,"-","-",5.5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL12AR270M9C01B0",106,265,"Vrms.",200,150,"-",310,360,"-",27,20,20,1.5,14,"-","-",6.5,"-","-",10,1.5,1.5,0.65,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL12AR150H8B72B0",106,265,"Vrms.",210,165,"-",400,460,"-",15,25,25,1.5,12.5,"-","-",6,"-","-",7.5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL12AR150H8B74B0",106,265,"Vrms.",210,165,"-",400,460,"-",15,25,25,1.5,12.5,"-","-",6,"-","-",7.5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","Special specification type"]
["TDK/EPCOS","B59850C0120A570",106,265,"Vrms.",220,165,121.00000000000001,330,396,"-",10,20,20,2.2000000000000002,13.5,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Thinking","PPL16220*A2B7",106,270,"Vrms.",230,"-","-",500,"-","-",22,"-","-",8,"14to18","-","-","3.0to7.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL11H251H*E",106,265,"Vrms.",250,200,155,375,442.5,480,12,20,20,1.5,10.5,"-","-",5.5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL14AR180M9C01B0",107,265,"Vrms.",230,180,"-",380,440,"-",18,20,20,2,15.7,"-","-",6.5,"-","-",10,1.5,1.5,0.65,0.05,0.05,-20,60,"-","-","-"]
["TDK/EPCOS","B59850C0120A570",107,265,"Vrms.",220,165,121.00000000000001,330,396,"-",10,20,20,2.2000000000000002,13.5,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Thinking","PPL16220*A2B7",107,270,"Vrms.",230,"-","-",500,"-","-",22,"-","-",8,"14to18","-","-","3.0to7.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL11H251H*E",107,265,"Vrms.",250,200,155,375,442.5,480,12,20,20,1.5,10.5,"-","-",5.5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL13AR100H8B72B0",108,265,"Vrms.",260,200,"-",480,560,"-",10,25,25,2.2000000000000002,14,"-","-",6,"-","-",7.5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL13AR100H8B52B0",108,265,"Vrms.",260,200,"-",480,560,"-",10,25,25,2.2000000000000002,14,"-","-",6,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["Thinking","PPL16220*A2B7",108,270,"Vrms.",230,"-","-",500,"-","-",22,"-","-",8,"14to18","-","-","3.0to7.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Vishay","PTCCL13H281H*E",108,265,"Vrms.",280,224,173.6,420,495.59999999999997,537.6,11,20,20,1.8,12.5,"-","-",5.5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"*=B:Bulk T:Tape and reel"]
["Murata","PTGL18AR6R0H8B72B0",109,265,"Vrms.",380,300,"-",715,830,"-",6,25,25,4.0999999999999996,18.5,"-","-",6,"-","-",7.5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","-"]
["Murata","PTGL18AR6R0H8D76A0",109,265,"Vrms.",380,300,"-",715,830,"-",6,25,25,4.0999999999999996,18.5,"-","-",6,"-","-","-","-","-",0.8,"-","-",-10,60,"-","-","Special specification type"]
["TDK/EPCOS","B59840C0120A070",109,265,"Vrms.",330,247.5,181.50000000000003,660,792,"-",6,25,25,4.0999999999999996,17.5,"-","-",5,"-","-",5,"-","-",0.6,"-","-",0,60,-40,125,"-"]
["Vishay","PTCCL17H401HBE",109,265,"Vrms.",400,320,248,600,708,768,6.6,20,20,3,16.5,"-","-",5.5,"-","-",5,"-","-",0.6,0.05,0.05,0,70,-40,175,"Bulk"]
["Murata","PTGL07AS251H0B51A0",110,280,"Vrms.","-",38,"-","-",90,"-",250,25,25,1.5,8,"-","-",6,"-","-",5,0.3,0.8,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL07AS251H0B51B0",110,280,"Vrms.","-",38,"-","-",90,"-",250,25,25,1.5,8,"-","-",6,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"-"]
["Murata","PTGL07AS251H0B54B1",110,280,"Vrms.","-",38,"-","-",90,"-",250,25,25,1.5,8,"-","-",6,"-","-",5,1.5,1.5,0.6,0.05,0.05,-30,85,-40,125,"Special specification type"]
["TDK/EPCOS","B59772C0120A070",110,260,"Vrms.",43,32.25,23.650000000000002,86,103.2,"-",150,25,25,2.8,9,"-","-",7.5,"-","-",5,"-","-",0.6,"-","-",-20,85,-40,125,"-"]
["Thinking","PPL11800*A2C8 ",110,380,"Vrms.",69,"-","-",137,"-","-",80,"-","-",2,"10.5to13","-","-","4.5to7.0","-","-",5,1,1,0.6,0.02,0.02,0,60,-25,125,"*= Resistance Torelance ex.) M,H,N"]
["Murata","PTGL07AM1R0M1B51A0",111,16,"Vrms.",700,"-","-",1200,"-","-",1,20,20,5,6.8,0.5,0.5,2.4,0.6,0.6,5,0.3,0.8,0.6,0.05,0.05,-40,85,"-","-","Special specification type"]
["Murata","PTGL07AM1R0M1B51B0",111,16,"Vrms.",700,"-","-",1200,"-","-",1,20,20,5,6.8,0.5,0.5,2.4,0.6,0.6,5,1.5,1.5,0.6,0.05,0.05,-40,85,"-","-","Special specification type"]
["Murata","PTGL07AM1R0M1B51B1",111,14,"Vrms.",650,"-","-",1150,"-","-",1,20,20,5,6.3,0.5,0.5,3,"-","-",5,1.5,1.5,0.6,0.05,0.05,-40,85,"-","-","Special specification type"]
[null,"該当品種無し(Non)",111]
["Murata","PTGL7SBD220H1P54BW",112,16,"VDC","-","-","-","-","-","-",22,30,30,1.5,6.7,0.7,0.7,2.5,0.5,0.5,5,1.5,1.5,0.6,0.05,0.05,-40,85,"-","-","Special specification type"]
[null,"該当品種無し(Non)",112]
["Murata","PTGL12ARR23N1C51A0",113,16,"Vrms.","-",1000,"-","-",3250,"-",0.23,30,30,7,12,"-","-",4,"-","-",5,0.3,0.8,0.65,"-","-",-30,85,"-","-","Special specification type"]
["Murata","PTGL12ARR23N1C51B0",113,16,"Vrms.","-",1000,"-","-",3250,"-",0.23,30,30,7,12,"-","-",4,"-","-",5,0.3,0.8,0.65,"-","-",-30,85,"-","-","Special specification type"]
[null,"該当品種無し(Non)",113]
["Murata","PTGL07AR150M5B51A0",114,85,"Vrms.","-","-","-","-","-","-",15,20,20,1,8.5,"-","-",5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","Special specification type"]
["Murata","PTGL07AR150M5B51B0",114,85,"Vrms.","-","-","-","-","-","-",15,20,20,1,8.5,"-","-",5,"-","-",5,1.5,1.5,0.6,0.05,0.05,-10,60,"-","-","Special specification type"]
[null,"該当品種無し(Non)",114]
["Murata","PTGL09AR8R5M5B51A9",115,85,"Vrms.","-","-","-","-","-","-",8.5,20,20,1.5,10.5,"-","-",5.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","Special specification type"]
["Murata","PTGL09AR8R5M5B51A0",115,85,"Vrms.","-","-","-","-","-","-",8.5,20,20,1.5,10.5,"-","-",5.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","Special specification type"]
[null,"該当品種無し(Non)",115]
["Murata","PTGL10AR6R5M5B52A0",116,85,"Vrms.","-","-","-","-","-","-",6.5,20,20,2,12,"-","-",5.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","Special specification type"]
["Murata","PTGL10AR6R5M5B52B0",116,85,"Vrms.","-","-","-","-","-","-",6.5,20,20,2,12,"-","-",5.5,"-","-",5,0.3,0.8,0.6,0.05,0.05,-10,60,"-","-","Special specification type"]
[null,"該当品種無し(Non)",116]
["Murata","PTGL7SBB122N0P03B2",117,500,"VDC","-","-",3,"-","-",31,1200,30,30,2.2000000000000002,7.4,"-","-",6.5,"-","-",10,1,1,0.6,0.05,0.05,-40,95,"-","-","Special specification type"]
[null,"該当品種無し(Non)",117]
["Murata","PTGL5SAR181M9P03B1",118,265,"Vrms.","-","-",25,"-","-",97,180,20,20,0.3,6.5,"-","-",6.5,"-","-",10,1,1,0.6,0.05,0.05,-30,85,"-","-","Special specification type"]
["Murata","PTGL5SAR181M9P03B2",118,265,"Vrms.","-",36,"-","-","90min.","-",180,20,20,0.3,6.5,"-","-",6.5,"-","-",10,1,1,0.6,0.05,0.05,-30,85,"-","-","Special specification type"]
["Murata","PTGL5SAR181M9P03BL",118,265,"Vrms.","-","-",25,"-","-",97,180,20,20,0.3,6.5,"-","-",6.5,"-","-",10,1,1,0.6,0.05,0.05,-30,85,"-","-","Special specification type"]
["Murata","PTGL05AR181M9P09B0",118,265,"Vrms.","-",36,"-","-","90min.","-",180,20,20,0.3,6.5,"-","-",6.5,"-","-",10,1,1,0.6,0.05,0.05,-30,85,"-","-","Special specification type"]
["Murata","PTGL5SAR181M9P09B0",118,265,"Vrms.","-",36,"-","-","90min.","-",180,20,20,0.3,6.5,"-","-",6.5,"-","-",10,1,1,0.6,0.05,0.05,-30,85,"-","-","Special specification type"]
[null,"該当品種無し(Non)",118,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]

{"sheet":"品番一覧","index":1,"n_rows":351,"n_cols":3,"rows_kept":351,"cut":false,"hidden":true,"merged":[]}
["メーカー\nMaker","品番\nPart Number","グルーピング"]
["Murata","PTGL03AR2R0Q1B53A0",3]
["Murata","PTGL03AR2R0Q1B53B0",3]
["Murata","PTGL04AR130H2B51A0",23]
["Murata","PTGL04AR130H2B51B0",23]
["Murata","PTGL04AS100K2B51A0",24]
["Murata","PTGL04AS100K2B51A0",24]
["Murata","PTGL04AS100K2B51B0",24]
["Murata","PTGL04AS100K2B51B0",24]
["Murata","PTGL04AS100K2B52AL",24]
["Murata","PTGL04AS100K2N51A0",21]
["Murata","PTGL04AS100K2N51B0",21]
["Murata","PTGL04AS100K2N51B1",21]
["Murata","PTGL04AS100K2N52AL",21]
["Murata","PTGL04AS100K3B51A0",40]
["Murata","PTGL04AS100K3B51B0",40]
["Murata","PTGL04AS100M2N51A0",21]
["Murata","PTGL04AS100M2N51B0",21]
["Murata","PTGL04AS220K4B51A0",56]
["Murata","PTGL04AS220K4B51B0",56]
["Murata","PTGL04AS220K4N51A0",57]
["Murata","PTGL04AS220K4N51B0",57]
["Murata","PTGL04AS220K4N52AL",57]
["Murata","PTGL04AS560K6B51A0",70]
["Murata","PTGL04AS560K6B51B0",70]
["Murata","PTGL04AS560K6B52AL",70]
["Murata","PTGL05AR121M9N51A0",93]
["Murata","PTGL05AR121M9N51B0",93]
["Murata","PTGL05AR121M9N51B1",93]
["Murata","PTGL05AR151H8P52A0",94]
["Murata","PTGL05AR151H8P52B0",94]
["Murata","PTGL05AR181M7N52A0",67]
["Murata","PTGL05AR181M7P52A0",67]
["Murata","PTGL05AR181M7P52B0",67]
["Murata","PTGL05AR181M9N51B0",95]
["Murata","PTGL05AR181M9N51B1",95]
["Murata","PTGL05AR181M9N51B2",95]
["Murata","PTGL05AR181M9N52A0",95]
["Murata","PTGL05AR181M9N52B0",95]
["Murata","PTGL05AR181M9P09B0",118]
["Murata","PTGL05AR1R0M1B51A0",5]
["Murata","PTGL05AR1R0M1B51B0",5]
["Murata","PTGL05AR301M7N52B0",89]
["Murata","PTGL05AR331M7A52B0",89]
["Murata","PTGL05AR550H4P51A0",64]
["Murata","PTGL05AR550H4P51B0",64]
["Murata","PTGL05AS100K4B51A0",58]
["Murata","PTGL05AS100K4B51B0",58]
["Murata","PTGL05AS270K6B51A0",72]
["Murata","PTGL05AS270K6B51B0",72]
["Murata","PTGL05AS3R9K2B51A0",22]
["Murata","PTGL05AS3R9K2B51B0",22]
["Murata","PTGL05AS3R9K2B51B2",22]
["Murata","PTGL05AS6R8K3B51A0",41]
["Murata","PTGL05AS6R8K3B51B0",41]
["Murata","PTGL05BA1R8M1B51A0",2]
["Murata","PTGL05BA1R8M1B51B0",2]
["Murata","PTGL05BD102N9N51A0",96]
["Murata","PTGL05BD102N9N51B0",96]
["Murata","PTGL05BD102N9N52A0",96]
["Murata","PTGL05BD102N9N52B0",96]
["Murata","PTGL06AR0R8M1B51A0",6]
["Murata","PTGL06AR0R8M1B51B0",6]
["Murata","PTGL06BB220N8B52A0",90]
["Murata","PTGL06BB220N8B52B0",90]
["Murata","PTGL07AM1R0M1B51A0",111]
["Murata","PTGL07AM1R0M1B51B0",111]
["Murata","PTGL07AM1R0M1B51B0",111]
["Murata","PTGL07AM1R0M1B51B1",111]
["Murata","PTGL07AR150M5B51A0",114]
["Murata","PTGL07AR150M5B51B0",114]
["Murata","PTGL07AR220M3N54B0",46]
["Murata","PTGL07AR220M3N54B0",46]
["Murata","PTGL07AR220M3N54B0",46]
["Murata","PTGL07AR220M3P51A0",48]
["Murata","PTGL07AR220M3P51B0",48]
["Murata","PTGL07AR250H4B51A0",65]
["Murata","PTGL07AR250H4B51B0",65]
["Murata","PTGL07AR330M6A51B0",71]
["Murata","PTGL07AR330M6A54B3",71]
["Murata","PTGL07AR330M6B51A0",71]
["Murata","PTGL07AR450H8B52A0",102]
["Murata","PTGL07AR450H8B52B0",102]
["Murata","PTGL07AR470M3B51A0",47]
["Murata","PTGL07AR470M3B51B0",47]
["Murata","PTGL07AR470M3B54B0",47]
["Murata","PTGL07AR4R6H2B51A0",25]
["Murata","PTGL07AR4R6H2B51B0",25]
["Murata","PTGL07AR4R7M2P51A0",36]
["Murata","PTGL07AR4R7M2P51B0",36]
["Murata","PTGL07AR560M9A51B0",101]
["Murata","PTGL07AR560M9A52B0",101]
["Murata","PTGL07AR560M9A54B0",101]
["Murata","PTGL07AR560M9B51A0",101]
["Murata","PTGL07AR650H8B52A0",98]
["Murata","PTGL07AR650H8B52B0",98]
["Murata","PTGL07AR680M3B51A0",45]
["Murata","PTGL07AR680M3B51B0",45]
["Murata","PTGL07AR6R8M2B51A0",39]
["Murata","PTGL07AR6R8M2B51B0",39]
["Murata","PTGL07AR700H8B52A0",100]
["Murata","PTGL07AR700H8B52B0",100]
["Murata","PTGL07AR700H8B52B1",100]
["Murata","PTGL07AR820M9A51B0",99]
["Murata","PTGL07AR820M9B51A0",99]
["Murata","PTGL07AR820M9B52A0",99]
["Murata","PTGL07AR8R2M3N54B0",50]
["Murata","PTGL07AR8R2M3P51A0",49]
["Murata","PTGL07AR8R2M3P51B0",49]
["Murata","PTGL07ARR47M1B51A0",8]
["Murata","PTGL07ARR47M1B51B0",8]
["Murata","PTGL07AS150K6B51A0",73]
["Murata","PTGL07AS150K6B51B0",73]
["Murata","PTGL07AS150K6B52AL",73]
["Murata","PTGL07AS150K6B54B0",73]
["Murata","PTGL07AS1R8K2B51A0",28]
["Murata","PTGL07AS1R8K2B51B0",28]
["Murata","PTGL07AS201M0N51A0",97]
["Murata","PTGL07AS201M0N51B0",97]
["Murata","PTGL07AS251H0B51A0",110]
["Murata","PTGL07AS251H0B51B0",110]
["Murata","PTGL07AS251H0B54B1",110]
["Murata","PTGL07AS2R7K2B51A0",26]
["Murata","PTGL07AS2R7K2B51B0",26]
["Murata","PTGL07AS3R3K3B51A0",42]
["Murata","PTGL07AS3R3K3B51B0",42]
["Murata","PTGL07AS3R3K3B52AL",42]
["Murata","PTGL07AS5R6K4B51A0",60]
["Murata","PTGL07AS5R6K4B51B0",60]
["Murata","PTGL07AS5R6K4N51A0",59]
["Murata","PTGL07AS5R6K4N51B0",59]
["Murata","PTGL07AS5R6K4N52AL",59]
["Murata","PTGL07BA0R9M1B51A0",7]
["Murata","PTGL07BA0R9M1B51B0",7]
["Murata","PTGL07BB220N0B52A0",91]
["Murata","PTGL07BB220N0B52B0",91]
["Murata","PTGL07BD150N3B51A0",35]
["Murata","PTGL07BD150N3B51B0",35]
["Murata","PTGL07BD200Q3B31A9",34]
["Murata","PTGL07BD220N3B51A0",34]
["Murata","PTGL07BD220N3B51B0",34]
["Murata","PTGL07BD330N3B51A0",33]
["Murata","PTGL07BD330N3B51B0",33]
["Murata","PTGL07BD330N3B51B9",33]
["Murata","PTGL07BD6R8N2B51A0",17]
["Murata","PTGL07BD6R8N2B51B0",17]
["Murata","PTGL09AR150M3B51A0",51]
["Murata","PTGL09AR150M3B51B0",51]
["Murata","PTGL09AR150M3B54B0",51]
["Murata","PTGL09AR1R8H2B51A0",27]
["Murata","PTGL09AR1R8H2B51B0",27]
["Murata","PTGL09AR1R8H2B51B9",27]
["Murata","PTGL09AR220M6B52A0",68]
["Murata","PTGL09AR220M6B52B0",68]
["Murata","PTGL09AR220M6C61B0",74]
["Murata","PTGL09AR250H8B52A0",105]
["Murata","PTGL09AR250H8B52B0",105]
["Murata","PTGL09AR250H8B52B1",105]
["Murata","PTGL09AR250H8B62B0",105]
["Murata","PTGL09AR2R7M2B51A0",20]
["Murata","PTGL09AR2R7M2B51B0",20]
["Murata","PTGL09AR390M9C61B0",104]
["Murata","PTGL09AR390N0B51A0",103]
["Murata","PTGL09AR390N0B52A0",103]
["Murata","PTGL09AR3R9M3B51A0",38]
["Murata","PTGL09AR3R9M3B51B0",38]
["Murata","PTGL09AR3R9M3P51A0",37]
["Murata","PTGL09AR3R9M3P51B0",37]
["Murata","PTGL09AR4R7M3B51A0",53]
["Murata","PTGL09AR4R7M3B51B0",53]
["Murata","PTGL09AR4R7M3C64B0",53]
["Murata","PTGL09AR8R5M5B51A0",115]
["Murata","PTGL09AR8R5M5B51A9",115]
["Murata","PTGL09AR9R4H4B51A0",66]
["Murata","PTGL09AR9R4H4B51B0",66]
["Murata","PTGL09ARR33M1B51A0",13]
["Murata","PTGL09ARR33M1B51B0",13]
["Murata","PTGL09AS120K6B51A0",76]
["Murata","PTGL09AS120K6B51B0",76]
["Murata","PTGL09AS120K6B74B1",76]
["Murata","PTGL09AS1R2K2B51A0",30]
["Murata","PTGL09AS1R2K2B51B0",30]
["Murata","PTGL09AS2R2K3B51A0",43]
["Murata","PTGL09AS2R2K3B51B0",43]
["Murata","PTGL09AS2R2K3B52AL",43]
["Murata","PTGL09AS3R3K4B51A0",62]
["Murata","PTGL09AS3R3K4B51B0",62]
["Murata","PTGL09AS3R3K4B74B1",62]
["Murata","PTGL09AS5R0K4B74B1",61]
["Murata","PTGL09AS7R6K6B51A0",78]
["Murata","PTGL09AS7R6K6B51B0",78]
["Murata","PTGL09AS7R6K6B74B1",78]
["Murata","PTGL09BA0R5M1B51A0",10]
["Murata","PTGL09BA0R5M1B51B0",10]
["Murata","PTGL09BA0R5M1P51B0",11]
["Murata","PTGL09BD3R3N2B51A0",19]
["Murata","PTGL09BD3R3N2B51B0",19]
["Murata","PTGL09BD4R7N2B51A0",18]
["Murata","PTGL09BD4R7N2B51B0",18]
["Murata","PTGL10AR150M6C61B0",75]
["Murata","PTGL10AR150M6C64B0",75]
["Murata","PTGL10AR3R9M3B51A0",54]
["Murata","PTGL10AR3R9M3B51B0",54]
["Murata","PTGL10AR3R9M3C61B0",54]
["Murata","PTGL10AR3R9M3C64B0",54]
["Murata","PTGL10AR3R9M3N64B0",52]
["Murata","PTGL10AR3R9M3P51A0",52]
["Murata","PTGL10AR3R9M3P51B0",52]
["Murata","PTGL10AR6R5M5B52A0",116]
["Murata","PTGL10AR6R5M5B52B0",116]
["Murata","PTGL10ARR27M1B51A0",14]
["Murata","PTGL10ARR27M1B51B0",14]
["Murata","PTGL10ARR27M1B51B1",14]
["Murata","PTGL10BB120N0P52A0",92]
["Murata","PTGL12AR0R2M1B51A0",15]
["Murata","PTGL12AR0R2M1B51B0",15]
["Murata","PTGL12AR100M6C01B0",79]
["Murata","PTGL12AR100M6C52B0",79]
["Murata","PTGL12AR150H8B72B0",106]
["Murata","PTGL12AR150H8B74B0",106]
["Murata","PTGL12AR1R2H2B51B0",29]
["Murata","PTGL12AR1R2M2A64B0",9]
["Murata","PTGL12AR1R2M2B51A0",9]
["Murata","PTGL12AR1R2M2B51B0",9]
["Murata","PTGL12AR270M9C01B0",106]
["Murata","PTGL12ARR23N1C51A0",113]
["Murata","PTGL12ARR23N1C51B0",113]
["Murata","PTGL12AS0R8K2B51A0",31]
["Murata","PTGL12AS0R8K2B51B0",31]
["Murata","PTGL12AS100Q6B74B2",77]
["Murata","PTGL12AS1R2K3B51A0",44]
["Murata","PTGL12AS1R2K3B51B0",44]
["Murata","PTGL12AS2R2K4B51A0",63]
["Murata","PTGL12AS2R2K4B51B0",63]
["Murata","PTGL12AS2R2K4B52AL",63]
["Murata","PTGL12AS4R7K6B51A0",81]
["Murata","PTGL12AS4R7K6B51B0",81]
["Murata","PTGL12AS4R7K6B52A0",81]
["Murata","PTGL12AS4R7K6B74B2",81]
["Murata","PTGL12AS6R0K6B04B2",80]
["Murata","PTGL12AS6R0K6B74B2",80]
["Murata","PTGL12AS6R3K6B74B2",80]
["Murata","PTGL12AS8R0K6B74B2",80]
["Murata","PTGL12AS9R0K6B04B2",77]
["Murata","PTGL12BA0R3H1B51A0",14]
["Murata","PTGL12BA0R3H1B51B0",14]
["Murata","PTGL13AR0R8H2B71B0",32]
["Murata","PTGL13AR0R9M1N04B0",12]
["Murata","PTGL13AR100H8B52B0",108]
["Murata","PTGL13AR100H8B72B0",108]
["Murata","PTGL13AR1R0M1C01B0",12]
["Murata","PTGL13AR1R0M1C04B0",12]
["Murata","PTGL13AR6R8M6C01B0",81]
["Murata","PTGL14AR100M6B72B0",69]
["Murata","PTGL14AR180M9C01B0",107]
["Murata","PTGL14AR3R3M3B71B0",55]
["Murata","PTGL14AR3R3M3C01B0",55]
["Murata","PTGL14AR3R3M3C04B0",55]
["Murata","PTGL14ARR15M1B51B0",16]
["Murata","PTGL14BA0R2H1B71B0",15]
["Murata","PTGL14BA0R2H1B74B0",15]
["Murata","PTGL16AR5R6M6C01B0",89]
["Murata","PTGL16AR5R6M6C01B3",89]
["Murata","PTGL16AR5R6M6C04B2",89]
["Murata","PTGL18AR6R0H8B72B0",109]
["Murata","PTGL18AR6R0H8D76A0",109]
["Murata","PTGL3SAR1R8K1E51A0",1]
["Murata","PTGL3SAR1R8M1E51A0",1]
["Murata","PTGL3SAR2R5M1N51A0",4]
["Murata","PTGL3SAR2R5M1N51B0",4]
["Murata","PTGL3SAR2R5M1N53A0",4]
["Murata","PTGL3SAR2R5M1N53B0",4]
["Murata","PTGL4SAS100K2B51A0",24]
["Murata","PTGL4SAS100K2B51B0",24]
["Murata","PTGL4SAS100K2B51B1",24]
["Murata","PTGL4SAS100K2N51A0",21]
["Murata","PTGL4SAS100K2N51B0",21]
["Murata","PTGL4SAS100K3B51A0",40]
["Murata","PTGL4SAS100K3B51B0",40]
["Murata","PTGL4SAS220K4B51A0",56]
["Murata","PTGL4SAS220K4B51B0",56]
["Murata","PTGL4SAS220K4N51A0",57]
["Murata","PTGL4SAS220K4N51B0",57]
["Murata","PTGL4SAS560K6B51A0",70]
["Murata","PTGL4SAS560K6B51B0",70]
["Murata","PTGL5SAR181M9P03B1",118]
["Murata","PTGL5SAR181M9P03B2",118]
["Murata","PTGL5SAR181M9P03BL",118]
["Murata","PTGL5SAR181M9P09B0",118]
["Murata","PTGL5SAR1R0M1B51A0",5]
["Murata","PTGL5SAR1R0M1B51B0",5]
["Murata","PTGL5SAR1R0M1B53A0",5]
["Murata","PTGL5SAR1R0M1B53B0",5]
["Murata","PTGL5SAS100K4B51A0",58]
["Murata","PTGL5SAS100K4B51B0",58]
["Murata","PTGL5SAS270K6B51A0",72]
["Murata","PTGL5SAS270K6B51B0",72]
["Murata","PTGL5SAS3R9K2B51A0",22]
["Murata","PTGL5SAS3R9K2B51B0",22]
["Murata","PTGL5SAS6R8K3B51A0",41]
["Murata","PTGL5SAS6R8K3B51B0",41]
["Murata","PTGL6SAR0R8M1B51A0",6]
["Murata","PTGL6SAR0R8M1B51B0",6]
["Murata","PTGL6SAR0R8M1B54B1",6]
["Murata","PTGL7SARR47M1B51A0",8]
["Murata","PTGL7SARR47M1B51B0",8]
["Murata","PTGL7SARR47M1N51A0",8]
["Murata","PTGL7SARR47M1N51B0",8]
["Murata","PTGL7SAS150K6B51A0",73]
["Murata","PTGL7SAS150K6B51B0",73]
["Murata","PTGL7SAS1R8K2B51A0",28]
["Murata","PTGL7SAS1R8K2B51B0",28]
["Murata","PTGL7SAS2R7K2B51A0",26]
["Murata","PTGL7SAS2R7K2B51B0",26]
["Murata","PTGL7SAS3R3K3B51A0",42]
["Murata","PTGL7SAS3R3K3B51B0",42]
["Murata","PTGL7SAS5R6K4B51A0",60]
["Murata","PTGL7SAS5R6K4B51B0",60]
["Murata","PTGL7SAS5R6K4N51A0",59]
["Murata","PTGL7SAS5R6K4N51B0",59]
["Murata","PTGL7SBB122N0P03B2",117]
["Murata","PTGL7SBD220H1P54BW",112]
["Murata","PTGL9SARR33M1B51A0",13]
["Murata","PTGL9SARR33M1B51B0",13]
["Murata","PTGL9SARR33M1B54B1",13]
["Murata","PTGL9SAS120K6B51A0",76]
["Murata","PTGL9SAS120K6B51B0",76]
["Murata","PTGL9SAS1R2K2B51A0",30]
["Murata","PTGL9SAS1R2K2B51B0",30]
["Murata","PTGL9SAS2R2K3B51A0",43]
["Murata","PTGL9SAS2R2K3B51B0",43]
["Murata","PTGL9SAS3R3K4B51A0",62]
["Murata","PTGL9SAS3R3K4B51B0",62]
["Murata","PTGL9SAS7R6K6B51A0",78]
["Murata","PTGL9SAS7R6K6B51B0",78]
["Murata","PTGLASARR27M1B51A0",14]
["Murata","PTGLASARR27M1B51B0",14]
["Murata","PTGLCSAR0R2M1B51A0",15]
["Murata","PTGLCSAR0R2M1B51B0",15]
["Murata","PTGLCSAR0R2M1B54B1",15]
["Murata","PTGLCSAS0R8K2B51A0",31]
["Murata","PTGLCSAS0R8K2B51B0",31]
["Murata","PTGLCSAS1R2K3B51A0",44]
["Murata","PTGLCSAS1R2K3B51B0",44]
["Murata","PTGLCSAS1R2K3B51B1",44]
["Murata","PTGLCSAS2R2K4B51A0",63]
["Murata","PTGLCSAS2R2K4B51B0",63]
["Murata","PTGLCSAS4R7K6B51A0",81]
["Murata","PTGLCSAS4R7K6B51B0",81]
["Murata","PTGLESARR15M1B51A0",16]
["Murata","PTGLESARR15M1B51B0",16]